| eMD IIM4265x Driver API 1.0.0

Here is a list of all struct and union fields with links to the structures/unions they belong to:

### - a -

- acc_ln_bw : inv_ixm42xxx
- acc_lp_avg : inv_ixm42xxx
- accel : inv_ixm42xxx_sensor_event_t
- accel_bit : fifo_header_t
- accel_cfg_0_reg : inv_ixm42xxx_transport::register_cache
- accel_config0 : recover_regs
- accel_config1 : recover_regs
- accel_gyro_config0 : recover_regs
- accel_high_res : inv_ixm42xxx_sensor_event_t
- accel_odr_different : fifo_header_t
- accel_st_bias : inv_ixm42xxx
- accel_start_time_us : inv_ixm42xxx
- activity_class : inv_ixm42xxx_apex_step_activity
- avg_bw_setting : inv_ixm42xxx

### - b -

- bank_sel_reg : inv_ixm42xxx_transport::register_cache
- bits : fifo_header_t
- Byte : fifo_header_t

### - c -

- configure : inv_ixm42xxx_serif
- context : inv_ixm42xxx_serif

### - d -

- dmp_is_on : inv_ixm42xxx
- double_tap_timing : inv_ixm42xxx_tap_data

### - e -

- endianess_data : inv_ixm42xxx

### - f -

- fifo_config1 : recover_regs
- fifo_data : inv_ixm42xxx
- fifo_highres_enabled : inv_ixm42xxx
- fifo_is_used : inv_ixm42xxx
- fsync_bit : fifo_header_t
- fsync_to_be_ignored : inv_ixm42xxx

### - g -

- gyr_ln_bw : inv_ixm42xxx
- gyro : inv_ixm42xxx_sensor_event_t
- gyro_bit : fifo_header_t
- gyro_cfg_0_reg : inv_ixm42xxx_transport::register_cache
- gyro_config0 : recover_regs
- gyro_config1 : recover_regs
- gyro_high_res : inv_ixm42xxx_sensor_event_t
- gyro_odr_different : fifo_header_t
- gyro_power_off_tmst : inv_ixm42xxx
- gyro_st_bias : inv_ixm42xxx
- gyro_start_time_us : inv_ixm42xxx

### - i -

- intf_cfg_1_reg : inv_ixm42xxx_transport::register_cache
- intf_config1 : recover_regs
- INV_IXM42XXX_FIFO_FULL : inv_ixm42xxx_interrupt_parameter_t
- INV_IXM42XXX_FIFO_THS : inv_ixm42xxx_interrupt_parameter_t
- INV_IXM42XXX_SLEEP_DET : inv_ixm42xxx_interrupt_parameter_t
- INV_IXM42XXX_SMD : inv_ixm42xxx_interrupt_parameter_t
- INV_IXM42XXX_STEP_CNT_OVFL : inv_ixm42xxx_interrupt_parameter_t
- INV_IXM42XXX_STEP_DET : inv_ixm42xxx_interrupt_parameter_t
- INV_IXM42XXX_TAP_DET : inv_ixm42xxx_interrupt_parameter_t
- INV_IXM42XXX_TILT_DET : inv_ixm42xxx_interrupt_parameter_t
- INV_IXM42XXX_UI_DRDY : inv_ixm42xxx_interrupt_parameter_t
- INV_IXM42XXX_UI_FSYNC : inv_ixm42xxx_interrupt_parameter_t
- INV_IXM42XXX_WAKE_DET : inv_ixm42xxx_interrupt_parameter_t
- INV_IXM42XXX_WOM_X : inv_ixm42xxx_interrupt_parameter_t
- INV_IXM42XXX_WOM_Y : inv_ixm42xxx_interrupt_parameter_t
- INV_IXM42XXX_WOM_Z : inv_ixm42xxx_interrupt_parameter_t

### - l -

- low_energy_amp_th : inv_ixm42xxx_apex_parameters

### - m -

- max_peak_tol : inv_ixm42xxx_tap_parameters_t
- max_read : inv_ixm42xxx_serif
- max_write : inv_ixm42xxx_serif
- min_jerk_thr : inv_ixm42xxx_tap_parameters_t
- msg_bit : fifo_header_t

### - p -

- pedo_amp_th : inv_ixm42xxx_apex_parameters
- pedo_hi_enrgy_th : inv_ixm42xxx_apex_parameters
- pedo_sb_timer_th : inv_ixm42xxx_apex_parameters
- pedo_step_cnt_th : inv_ixm42xxx_apex_parameters
- pedo_step_det_th : inv_ixm42xxx_apex_parameters
- power_save : inv_ixm42xxx_apex_parameters
- power_save_time : inv_ixm42xxx_apex_parameters
- pwr_mgmt_0 : recover_regs
- pwr_mngt_0_reg : inv_ixm42xxx_transport::register_cache

### - r -

- r2w_gest_delay : inv_ixm42xxx_apex_parameters
- r2w_mounting_matrix : inv_ixm42xxx_apex_parameters
- r2w_sleep_time_out : inv_ixm42xxx_apex_parameters
- read_reg : inv_ixm42xxx_serif
- register_cache : inv_ixm42xxx_transport
- reserved : inv_ixm42xxx

### - s -

- self_test_config : recover_regs
- sensitivity_mode : inv_ixm42xxx_apex_parameters
- sensor_event_cb : inv_ixm42xxx
- sensor_mask : inv_ixm42xxx_sensor_event_t
- serif : inv_ixm42xxx_transport
- serif_type : inv_ixm42xxx_serif
- st_result : inv_ixm42xxx
- step_cadence : inv_ixm42xxx_apex_step_activity
- step_cnt : inv_ixm42xxx_apex_step_activity

### - t -

- tap_axis : inv_ixm42xxx_tap_data
- tap_dir : inv_ixm42xxx_tap_data
- tap_num : inv_ixm42xxx_tap_data
- tavg : inv_ixm42xxx_tap_parameters_t
- temperature : inv_ixm42xxx_sensor_event_t
- tilt_wait_time : inv_ixm42xxx_apex_parameters
- timestamp_bit : fifo_header_t
- timestamp_fsync : inv_ixm42xxx_sensor_event_t
- tmax : inv_ixm42xxx_tap_parameters_t
- tmin : inv_ixm42xxx_tap_parameters_t
- tmst_cfg_reg : inv_ixm42xxx_transport::register_cache
- tmst_to_reg_en_cnt : inv_ixm42xxx
- transport : inv_ixm42xxx
- twentybits_bit : fifo_header_t

### - w -

- wom_enable : inv_ixm42xxx
- wom_smd_mask : inv_ixm42xxx
- write_reg : inv_ixm42xxx_serif
- wu_off_acc_odr_changes : inv_ixm42xxx