<map id="inv_ixm42xxx_set_reg_bank" name="inv_ixm42xxx_set_reg_bank">
<area shape="rect" id="node1" title="Set register bank index." alt="" coords="479,423,664,450"/>
<area shape="rect" id="node2" href="$group___driver_ixm42xxx_driver___h_l__apex.html#gaa50e8df22ed1e43ecb30f0c1d9c0c430" title="Configures DMP parameters for APEX algorithms (pedometer, tilt). This programmable parameters will be..." alt="" coords="254,5,413,47"/>
<area shape="rect" id="node3" href="$group___driver_ixm42xxx_driver___h_l__apex.html#gaf8ba3ca8d0678f27da5dca720ad7cb45" title="Configure Wake On Motion and SMD thresholds." alt="" coords="254,71,413,112"/>
<area shape="rect" id="node4" href="$group___driver_ixm42xxx_driver___h_l__apex.html#gad8b43a38f4373f472fbd38abcf160a50" title="Configure TAP." alt="" coords="254,136,413,177"/>
<area shape="rect" id="node5" href="$group___driver_ixm42xxx_driver___h_l.html#ga216741ead81e5df761808bf84ce7dd6a" title="Perform a soft reset of the device." alt="" coords="262,201,405,243"/>
<area shape="rect" id="node6" href="$group___driver_ixm42xxx_driver___h_l.html#ga0019ff7dabd81d8f251ba70c5a1e2149" title="Enable or disable CLKIN/RTC capability." alt="" coords="261,267,406,308"/>
<area shape="rect" id="node7" href="$group___driver_ixm42xxx_driver___h_l__apex.html#gaddf125e2656d936c5ab2b1cedd1e338a" title="Returns current DMP parameters for APEX algorithms (pedometer, tilt)." alt="" coords="253,332,413,373"/>
<area shape="rect" id="node8" href="$group___driver_ixm42xxx_driver___h_l.html#ga66c5185abd16d812763091b79a678616" title="Retrieve interrupts configuration." alt="" coords="240,499,427,526"/>
<area shape="rect" id="node12" href="$group___driver_ixm42xxx_driver___h_l.html#ga01d140f0c4cdd75e519b40c37f520a6b" title="Retrieve interrupts configuration." alt="" coords="236,601,431,627"/>
<area shape="rect" id="node14" href="$group___driver_ixm42xxx_driver___h_l.html#ga02d9e73649adc7063b87b528789da746" title="Retrieve interrupts configuration." alt="" coords="236,398,431,425"/>
<area shape="rect" id="node15" href="$group___driver_ixm42xxx_driver___h_l.html#gacbeebf144a933be15100e49360cc8e60" title="Get the timestamp value of ixm42xxx from register." alt="" coords="247,703,419,744"/>
<area shape="rect" id="node16" href="$group___driver_ixm42xxx_driver___h_l__apex.html#ga3691d1a69cd1b8ffec60b3e96d302c88" title="Returns current TAP parameters." alt="" coords="258,768,409,809"/>
<area shape="rect" id="node17" href="$group___driver_ixm42xxx_driver___h_l.html#gaffb6e096b26cce389121a6fcd33ad546" title="Configure which interrupt source can trigger ibi interruptions." alt="" coords="240,550,427,577"/>
<area shape="rect" id="node18" href="$group___driver_ixm42xxx_driver___h_l.html#ga14aafe11842b6f9df47e4ebe56334db9" title="Configure which interrupt source can trigger INT1." alt="" coords="236,651,431,678"/>
<area shape="rect" id="node19" href="$group___driver_ixm42xxx_driver___h_l.html#gaf17db67a06978d2e94dfff9684c513fe" title="Configure which interrupt source can trigger INT2." alt="" coords="236,449,431,475"/>
<area shape="rect" id="node9" href="$group___driver_ixm42xxx_driver___h_l.html#ga54b858024104c99002e06bf896d98362" title="Configure Fifo watermark (also refered to as fifo threshold)" alt="" coords="17,484,176,525"/>
<area shape="rect" id="node10" href="$group___driver_ixm42xxx_driver___h_l__apex.html#ga99c5ebe8e253e35c4aca839e1f2b2822" title="Disable Wake On Motion. Disables WoM event generation and reconfigures interrupt to fire on Fifo wate..." alt="" coords="5,550,188,577"/>
<area shape="rect" id="node11" href="$group___driver_ixm42xxx_driver___h_l__apex.html#gae966c458a6571d4292b57427283418e6" title="Enable Wake On Motion. note : WoM requests to have the accelerometer enabled to work...." alt="" coords="7,601,186,627"/>
<area shape="rect" id="node13" href="$group___driver_ixm42xxx_driver___h_l.html#ga86649a7a95e6ca5ceceb3d0663ea89d7" title="Configure Fifo to select the way data are gathered." alt="" coords="5,651,188,678"/>
</map>
