<map id="inv_ixm42xxx_write_reg" name="inv_ixm42xxx_write_reg">
<area shape="rect" id="node1" title="Writes data to a register on Ixm42xxx." alt="" coords="712,1338,871,1365"/>
<area shape="rect" id="node2" href="$group___driver_ixm42xxx_driver___h_l__apex.html#gaa50e8df22ed1e43ecb30f0c1d9c0c430" title="Configures DMP parameters for APEX algorithms (pedometer, tilt). This programmable parameters will be..." alt="" coords="254,78,413,119"/>
<area shape="rect" id="node3" href="$group___driver_ixm42xxx_driver___h_l.html#ga86649a7a95e6ca5ceceb3d0663ea89d7" title="Configure Fifo to select the way data are gathered." alt="" coords="5,774,188,801"/>
<area shape="rect" id="node4" href="$group___driver_ixm42xxx_driver___h_l.html#ga54b858024104c99002e06bf896d98362" title="Configure Fifo watermark (also refered to as fifo threshold)" alt="" coords="17,575,176,616"/>
<area shape="rect" id="node5" href="$group___driver_ixm42xxx_driver___h_l__apex.html#gaf8ba3ca8d0678f27da5dca720ad7cb45" title="Configure Wake On Motion and SMD thresholds." alt="" coords="254,143,413,184"/>
<area shape="rect" id="node6" href="$group___driver_ixm42xxx_driver___h_l__apex.html#gad8b43a38f4373f472fbd38abcf160a50" title="Configure TAP." alt="" coords="254,208,413,250"/>
<area shape="rect" id="node7" href="$group___driver_ixm42xxx_driver___h_l.html#ga2b4caf4abbe52a1c089b11eb316e5266" title="Configure timestamp resolution from FIFO." alt="" coords="492,72,651,114"/>
<area shape="rect" id="node8" href="$group___driver_ixm42xxx_driver___h_l.html#ga0019ff7dabd81d8f251ba70c5a1e2149" title="Enable or disable CLKIN/RTC capability." alt="" coords="261,12,406,54"/>
<area shape="rect" id="node9" href="$group___driver_ixm42xxx_driver___h_l.html#ga216741ead81e5df761808bf84ce7dd6a" title="Perform a soft reset of the device." alt="" coords="262,274,405,315"/>
<area shape="rect" id="node10" href="$group___driver_ixm42xxx_driver___h_l.html#ga300b49e3d242183d3dcc3102a3341f4c" title="Disable all 3 axes of accel." alt="" coords="259,966,407,1007"/>
<area shape="rect" id="node11" href="$group___driver_ixm42xxx_driver___h_l__apex.html#gaa4d835bb4917561299c67e426b5e243d" title="Disable APEX algorithm Pedometer." alt="" coords="497,1298,645,1339"/>
<area shape="rect" id="node12" href="$group___driver_ixm42xxx_driver___h_l__apex.html#gab66cfbfd0a46b2da0d6578c62862ded0" title="Disable APEX algorithm Raise to wake." alt="" coords="497,1363,645,1404"/>
<area shape="rect" id="node13" href="$group___driver_ixm42xxx_driver___h_l__apex.html#gaabbead373311aa012e29ce5a4f3a4271" title="Disable APEX algorithm Tilt." alt="" coords="497,1428,645,1470"/>
<area shape="rect" id="node14" href="$group___driver_ixm42xxx_driver___h_l.html#ga49491c47baf3acd453571583828be8a1" title="Disable fsync tagging functionnality. In details it:" alt="" coords="497,1494,645,1535"/>
<area shape="rect" id="node15" href="$group___driver_ixm42xxx_driver___h_l.html#gab965bf11dffb9bf6179fbc06654b2de9" title="Disable all 3 axes of gyro." alt="" coords="243,1032,423,1058"/>
<area shape="rect" id="node16" href="$group___driver_ixm42xxx_driver___h_l.html#ga1466aac83b31a4801d85f2bb71370486" title="Disable 20 bits raw acc and raw gyr data in fifo." alt="" coords="497,1559,645,1600"/>
<area shape="rect" id="node17" href="$group___driver_ixm42xxx_driver___h_l__apex.html#ga8d0a5a362e2bd1cf50dcea63afd40e1e" title="Disable Significant Motion Detection. Disables SMD event generation and disables SMD interrupt." alt="" coords="481,1625,661,1652"/>
<area shape="rect" id="node18" href="$group___driver_ixm42xxx_driver___h_l__apex.html#ga8d0314f16b61d66b8f427b2b14f6105f" title="Disable TAP." alt="" coords="485,1676,658,1702"/>
<area shape="rect" id="node19" href="$group___driver_ixm42xxx_driver___h_l.html#gad5eee9e5994aea633d8716de1c63920f" title="Disable the 20bits&#45;timestamp register access. Register read always return 0&#39;s." alt="" coords="492,1727,651,1768"/>
<area shape="rect" id="node20" href="$group___driver_ixm42xxx_driver___h_l__apex.html#ga99c5ebe8e253e35c4aca839e1f2b2822" title="Disable Wake On Motion. Disables WoM event generation and reconfigures interrupt to fire on Fifo wate..." alt="" coords="5,662,188,689"/>
<area shape="rect" id="node21" href="$group___driver_ixm42xxx_driver___h_l.html#gaee954cc3e40a2cf3cf92ffcf27c963dc" title="Enable/put accel in low noise mode." alt="" coords="252,1086,415,1127"/>
<area shape="rect" id="node22" href="$group___driver_ixm42xxx_driver___h_l.html#ga7d0afe076a89155fee929b3c083175ad" title="Enable/put accel in low power mode." alt="" coords="250,1156,417,1198"/>
<area shape="rect" id="node23" href="$group___driver_ixm42xxx_driver___h_l__apex.html#gace0ceae9fba5451c65b53e0429fea3b6" title="Enable APEX algorithm Pedometer. note : Pedometer request to have the accelerometer enabled to works ..." alt="" coords="499,1792,644,1834"/>
<area shape="rect" id="node24" href="$group___driver_ixm42xxx_driver___h_l__apex.html#gab2707d8384121f4fbdb206b8e3659c7b" title="Enable APEX algorithm Raise to wake. note : Raise to wake request to have the accelerometer enabled t..." alt="" coords="499,1858,644,1899"/>
<area shape="rect" id="node25" href="$group___driver_ixm42xxx_driver___h_l__apex.html#ga51f843bc5bc3712a81f1fddd7b88ed4b" title="Enable APEX algorithm Tilt. note : Tilt request to have the accelerometer enabled to works with accel..." alt="" coords="499,1923,644,1964"/>
<area shape="rect" id="node26" href="$group___driver_ixm42xxx_driver___h_l.html#ga8296de3d1334fd82b36f7d51eddfb3d4" title="Enable fsync tagging functionnality. In details it:" alt="" coords="499,1988,644,2030"/>
<area shape="rect" id="node27" href="$group___driver_ixm42xxx_driver___h_l.html#ga1fe26aa78d081ff6d2a19e18e25fa719" title="Enable/put gyro in low noise mode." alt="" coords="255,1232,412,1274"/>
<area shape="rect" id="node28" href="$group___driver_ixm42xxx_driver___h_l.html#ga3c0a0a45a3cd09f7ea94d35f291a6cf4" title="Enable 20 bits raw acc and raw gyr data in fifo." alt="" coords="499,2054,644,2095"/>
<area shape="rect" id="node29" href="$group___driver_ixm42xxx_driver___h_l__apex.html#gaab183ec40d9744683a79e969ba1ab7c5" title="Enable Significant Motion Detection. note : SMD requests to have the accelerometer enabled to work...." alt="" coords="483,2120,660,2146"/>
<area shape="rect" id="node30" href="$group___driver_ixm42xxx_driver___h_l__apex.html#gaace520a79ce8eac3d9bcd8585a77b4ab" title="Enable TAP. note : TAP requests to have the accelerometer enabled to work. To have good performance,..." alt="" coords="486,2170,657,2197"/>
<area shape="rect" id="node31" href="$group___driver_ixm42xxx_driver___h_l.html#ga3281240aeb8dda833588ce443629feb8" title="Enable the 20bits&#45;timestamp register access to read in a reliable way the strobed timestamp...." alt="" coords="492,2222,651,2263"/>
<area shape="rect" id="node32" href="$group___driver_ixm42xxx_driver___h_l__apex.html#gae966c458a6571d4292b57427283418e6" title="Enable Wake On Motion. note : WoM requests to have the accelerometer enabled to work...." alt="" coords="7,713,186,740"/>
<area shape="rect" id="node33" href="$group___driver_ixm42xxx_driver___h_l.html#gac62cde6e351bbc64c80183882fec8652" title="Configure Accel clock source." alt="" coords="504,1130,639,1171"/>
<area shape="rect" id="node34" href="$group___driver_ixm42xxx_driver___h_l.html#gacbeebf144a933be15100e49360cc8e60" title="Get the timestamp value of ixm42xxx from register." alt="" coords="247,339,419,380"/>
<area shape="rect" id="node35" href="$group___driver_ixm42xxx_driver___h_l.html#ga978d6a926ad4124c331c0463aeb15145" title="reset IXM42XXX fifo" alt="" coords="492,977,651,1004"/>
<area shape="rect" id="node36" href="$group___driver_ixm42xxx_driver___h_l.html#ga7307d038edc35d8b5ad3515c7ae34b47" title="Configure accel Output Data Rate." alt="" coords="490,2287,653,2328"/>
<area shape="rect" id="node37" href="$group___driver_ixm42xxx_driver___h_l.html#ga348d9e83a0924cbe8d7c6b7d704a5682" title="Set accel full scale range." alt="" coords="479,2353,663,2380"/>
<area shape="rect" id="node38" href="$group___driver_ixm42xxx_driver___h_l.html#gaafbf37269108bc14f498a121255afb7b" title="Set accel Low&#45;Noise bandwidth value." alt="" coords="490,2404,653,2446"/>
<area shape="rect" id="node39" href="$group___driver_ixm42xxx_driver___h_l.html#ga08e19a862fc06244b7e88de153e98b91" title="Set accel Low&#45;Power averaging value." alt="" coords="490,2470,653,2511"/>
<area shape="rect" id="node40" href="$group___driver_ixm42xxx_driver___h_l__apex.html#ga8d1670124cba662e89b211e3d530dc27" title="Configure DMP Output Data Rate for APEX algorithms (pedometer, tilt)" alt="" coords="491,2535,651,2576"/>
<area shape="rect" id="node41" href="$group___driver_ixm42xxx_driver___h_l.html#gaffb6e096b26cce389121a6fcd33ad546" title="Configure which interrupt source can trigger ibi interruptions." alt="" coords="240,622,427,649"/>
<area shape="rect" id="node42" href="$group___driver_ixm42xxx_driver___h_l.html#ga14aafe11842b6f9df47e4ebe56334db9" title="Configure which interrupt source can trigger INT1." alt="" coords="236,774,431,801"/>
<area shape="rect" id="node43" href="$group___driver_ixm42xxx_driver___h_l.html#gaf17db67a06978d2e94dfff9684c513fe" title="Configure which interrupt source can trigger INT2." alt="" coords="236,470,431,497"/>
<area shape="rect" id="node44" href="$group___driver_ixm42xxx_driver___h_l.html#ga90922ad19bd8d984c1130375e5638286" title="Configure gyro Output Data Rate." alt="" coords="493,2600,650,2642"/>
<area shape="rect" id="node45" href="$group___driver_ixm42xxx_driver___h_l.html#gad71c4a4e27f18b8d218acbd0db2673cc" title="Set gyro full scale range." alt="" coords="482,2666,661,2693"/>
<area shape="rect" id="node46" href="$group___driver_ixm42xxx_driver___h_l.html#ga2933d3c85ebb5019de2701812422fdb3" title="Set gyro Low&#45;Noise bandwidth value." alt="" coords="493,2718,650,2759"/>
<area shape="rect" id="node47" href="$group___driver_ixm42xxx_driver___h_l.html#ga8817386c1e4b5d4ee66238e2c6172f09" title="Set register bank index." alt="" coords="479,412,664,438"/>
<area shape="rect" id="node48" href="$group___driver_ixm42xxx_driver___h_l__apex.html#gaddf125e2656d936c5ab2b1cedd1e338a" title="Returns current DMP parameters for APEX algorithms (pedometer, tilt)." alt="" coords="253,404,413,446"/>
<area shape="rect" id="node49" href="$group___driver_ixm42xxx_driver___h_l.html#ga66c5185abd16d812763091b79a678616" title="Retrieve interrupts configuration." alt="" coords="240,572,427,598"/>
<area shape="rect" id="node50" href="$group___driver_ixm42xxx_driver___h_l.html#ga01d140f0c4cdd75e519b40c37f520a6b" title="Retrieve interrupts configuration." alt="" coords="236,673,431,700"/>
</map>
