<map id="inv_ixm42xxx_device_reset" name="inv_ixm42xxx_device_reset">
<area shape="rect" id="node1" title="Perform a soft reset of the device." alt="" coords="5,99,148,141"/>
<area shape="rect" id="node2" href="$group___driver_ixm42xxx_transport.html#gae8074e18d1a995e07d58ba52e8c4935e" title="Init cache variable." alt="" coords="197,5,380,32"/>
<area shape="rect" id="node3" href="$group___driver_ixm42xxx_transport.html#ga649560d180b5c0018269d3a83597acc6" title="Reads data from a register on Ixm42xxx." alt="" coords="210,56,367,83"/>
<area shape="rect" id="node4" href="$group___driver_ixm42xxx_driver___h_l.html#ga8817386c1e4b5d4ee66238e2c6172f09" title="Set register bank index." alt="" coords="196,107,381,133"/>
<area shape="rect" id="node5" href="$group___driver_ixm42xxx_transport.html#ga1ff0b8e2eb26c611b82e795b6653ff1a" title="Writes data to a register on Ixm42xxx." alt="" coords="429,132,588,159"/>
<area shape="rect" id="node6" href="$group___driver_ixm42xxx_ext.html#gac7b05db7fc2dcb42a571144e94a6355d" title="Hook for low&#45;level high res system sleep() function to be implemented by upper layer ~100us resolutio..." alt="" coords="209,208,368,235"/>
</map>
