| eMD IIM4265x Driver API 1.0.0

Data Fields
inv_ixm42xxx_transport::register_cache Struct Reference

Contains mirrored values of some IP registers. More...

`#include <Ixm42xxxTransport.h>`

## Data Fields
uint8_t | intf_cfg_1_reg
uint8_t | pwr_mngt_0_reg
uint8_t | gyro_cfg_0_reg
uint8_t | accel_cfg_0_reg
uint8_t | tmst_cfg_reg
uint8_t | bank_sel_reg

## Detailed Description

Contains mirrored values of some IP registers.

Definition at line 77 of file Ixm42xxxTransport.h.

## Field Documentation

## ◆ accel_cfg_0_reg

uint8_t accel_cfg_0_reg

ACCEL_CONFIG0, Bank: 0, Address: 0x50

Definition at line 81 of file Ixm42xxxTransport.h.

## ◆ bank_sel_reg

uint8_t bank_sel_reg

MPUREG_REG_BANK_SEL, All banks, Address 0x76

Definition at line 83 of file Ixm42xxxTransport.h.

## ◆ gyro_cfg_0_reg

uint8_t gyro_cfg_0_reg

GYRO_CONFIG0, Bank: 0, Address: 0x4F

Definition at line 80 of file Ixm42xxxTransport.h.

## ◆ intf_cfg_1_reg

uint8_t intf_cfg_1_reg

INTF_CONFIG1, Bank: 0, Address: 0x4D

Definition at line 78 of file Ixm42xxxTransport.h.

## ◆ pwr_mngt_0_reg

uint8_t pwr_mngt_0_reg

PWR_MGMT_0, Bank: 0, Address: 0x4E

Definition at line 79 of file Ixm42xxxTransport.h.

## ◆ tmst_cfg_reg

uint8_t tmst_cfg_reg

TMST_CONFIG, Bank: 0, Address: 0x54

Definition at line 82 of file Ixm42xxxTransport.h.

The documentation for this struct was generated from the following file:

- Ixm42xxxTransport.h