<map id="inv_ixm42xxx_set_config_int2" name="inv_ixm42xxx_set_config_int2">
<area shape="rect" id="node1" title="Configure which interrupt source can trigger INT2." alt="" coords="212,13,407,39"/>
<area shape="rect" id="node2" href="$group___driver_ixm42xxx_driver___h_l.html#ga54b858024104c99002e06bf896d98362" title="Configure Fifo watermark (also refered to as fifo threshold)" alt="" coords="5,5,164,47"/>
</map>
