| eMD IIM4265x Driver API 1.0.0

Data Structures
Here are the data structures with brief descriptions:
[detail level 1 2]

C fifo_header_t |
C inv_ixm42xxx | Ixm42xxx driver states definition
C inv_ixm42xxx_apex_parameters | Ixm42xxx APEX inputs parameters definition
C inv_ixm42xxx_apex_step_activity | APEX pedometer outputs
C inv_ixm42xxx_interrupt_parameter_t | Ixm42xxx set of interrupt enable flag
C inv_ixm42xxx_sensor_event_t | Sensor event structure definition
C inv_ixm42xxx_serif | Basesensor serial interface
C inv_ixm42xxx_tap_data | TAP outputs
C inv_ixm42xxx_tap_parameters_t | Ixm42xxx TAP inputs parameters definition
▼C inv_ixm42xxx_transport | Transport interface
C register_cache | Contains mirrored values of some IP registers
C recover_regs | Contains the current register values. Used to reapply values after the ST procedure