| eMD IIM4265x Driver API 1.0.0

Data Fields
inv_ixm42xxx_apex_step_activity Struct Reference
Ixm42xxx driver high level functions related to APEX

APEX pedometer outputs. More...

`#include <Ixm42xxxDriver_HL_apex.h>`

## Data Fields
uint16_t | step_cnt
uint8_t | step_cadence
uint8_t | activity_class

## Detailed Description

APEX pedometer outputs.

Definition at line 93 of file Ixm42xxxDriver_HL_apex.h.

## Field Documentation

## ◆ activity_class

uint8_t activity_class

Detected activity unknown (0), walk (1) or run (2)

Definition at line 97 of file Ixm42xxxDriver_HL_apex.h.

## ◆ step_cadence

uint8_t step_cadence

Walk/run cadency in number of samples. Format is u6.2. E.g, At 50Hz and 2Hz walk frequency, if the cadency is 25 samples. The register will output 100.

Definition at line 95 of file Ixm42xxxDriver_HL_apex.h.

## ◆ step_cnt

uint16_t step_cnt

Number of steps taken

Definition at line 94 of file Ixm42xxxDriver_HL_apex.h.

The documentation for this struct was generated from the following file:

- Ixm42xxxDriver_HL_apex.h