<map id="inv_ixm42xxx_enable_timestamp_to_register" name="inv_ixm42xxx_enable_timestamp_to_register">
<area shape="rect" id="node1" title="Enable the 20bits&#45;timestamp register access to read in a reliable way the strobed timestamp...." alt="" coords="5,49,164,90"/>
<area shape="rect" id="node2" href="$group___driver_ixm42xxx_transport.html#ga649560d180b5c0018269d3a83597acc6" title="Reads data from a register on Ixm42xxx." alt="" coords="213,5,370,32"/>
<area shape="rect" id="node3" href="$group___driver_ixm42xxx_ext.html#gac7b05db7fc2dcb42a571144e94a6355d" title="Hook for low&#45;level high res system sleep() function to be implemented by upper layer ~100us resolutio..." alt="" coords="212,56,371,83"/>
<area shape="rect" id="node4" href="$group___driver_ixm42xxx_transport.html#ga1ff0b8e2eb26c611b82e795b6653ff1a" title="Writes data to a register on Ixm42xxx." alt="" coords="212,107,371,133"/>
</map>
