<map id="inv_ixm42xxx_init" name="inv_ixm42xxx_init">
<area shape="rect" id="node1" title="Configure the serial interface used to access the device and execute hardware initialization." alt="" coords="5,5,129,32"/>
<area shape="rect" id="node2" href="$group___driver_ixm42xxx_ext.html#gac7b05db7fc2dcb42a571144e94a6355d" title="Hook for low&#45;level high res system sleep() function to be implemented by upper layer ~100us resolutio..." alt="" coords="177,5,336,32"/>
</map>
