| eMD IIM4265x Driver API 1.0.0

Data Fields
recover_regs Struct Reference

Contains the current register values. Used to reapply values after the ST procedure. More...

## Data Fields
uint8_t | intf_config1
uint8_t | pwr_mgmt_0
uint8_t | accel_config0
uint8_t | accel_config1
uint8_t | gyro_config0
uint8_t | gyro_config1
uint8_t | accel_gyro_config0
uint8_t | fifo_config1
uint8_t | self_test_config

## Detailed Description

Contains the current register values. Used to reapply values after the ST procedure.

Definition at line 77 of file Ixm42xxxSelfTest.c.

## Field Documentation

## ◆ accel_config0

uint8_t accel_config0

Definition at line 81 of file Ixm42xxxSelfTest.c.

## ◆ accel_config1

uint8_t accel_config1

Definition at line 82 of file Ixm42xxxSelfTest.c.

## ◆ accel_gyro_config0

uint8_t accel_gyro_config0

Definition at line 85 of file Ixm42xxxSelfTest.c.

## ◆ fifo_config1

uint8_t fifo_config1

Definition at line 86 of file Ixm42xxxSelfTest.c.

## ◆ gyro_config0

uint8_t gyro_config0

Definition at line 83 of file Ixm42xxxSelfTest.c.

## ◆ gyro_config1

uint8_t gyro_config1

Definition at line 84 of file Ixm42xxxSelfTest.c.

## ◆ intf_config1

uint8_t intf_config1

Definition at line 79 of file Ixm42xxxSelfTest.c.

## ◆ pwr_mgmt_0

uint8_t pwr_mgmt_0

Definition at line 80 of file Ixm42xxxSelfTest.c.

## ◆ self_test_config

uint8_t self_test_config

Definition at line 87 of file Ixm42xxxSelfTest.c.

The documentation for this struct was generated from the following file:

- Ixm42xxxSelfTest.c