<map id="inv_ixm42xxx_sleep_us" name="inv_ixm42xxx_sleep_us">
<area shape="rect" id="node1" title="Hook for low&#45;level high res system sleep() function to be implemented by upper layer ~100us resolutio..." alt="" coords="233,195,392,222"/>
<area shape="rect" id="node2" href="$group___driver_ixm42xxx_driver___h_l.html#ga216741ead81e5df761808bf84ce7dd6a" title="Perform a soft reset of the device." alt="" coords="24,5,167,47"/>
<area shape="rect" id="node3" href="$group___driver_ixm42xxx_driver___h_l.html#gab965bf11dffb9bf6179fbc06654b2de9" title="Disable all 3 axes of gyro." alt="" coords="5,71,185,98"/>
<area shape="rect" id="node4" href="$group___driver_ixm42xxx_driver___h_l.html#gaee954cc3e40a2cf3cf92ffcf27c963dc" title="Enable/put accel in low noise mode." alt="" coords="14,123,177,164"/>
<area shape="rect" id="node5" href="$group___driver_ixm42xxx_driver___h_l.html#ga7d0afe076a89155fee929b3c083175ad" title="Enable/put accel in low power mode." alt="" coords="12,188,179,229"/>
<area shape="rect" id="node6" href="$group___driver_ixm42xxx_driver___h_l.html#ga1fe26aa78d081ff6d2a19e18e25fa719" title="Enable/put gyro in low noise mode." alt="" coords="17,253,174,295"/>
<area shape="rect" id="node7" href="$group___driver_ixm42xxx_driver___h_l.html#ga3281240aeb8dda833588ce443629feb8" title="Enable the 20bits&#45;timestamp register access to read in a reliable way the strobed timestamp...." alt="" coords="16,319,175,360"/>
<area shape="rect" id="node8" href="$group___driver_ixm42xxx_driver___h_l.html#ga9476f939a18ccd3684b93ec493e04c31" title="Configure the serial interface used to access the device and execute hardware initialization." alt="" coords="33,385,157,411"/>
</map>
