<map id="inv_ixm42xxx_configure_fifo_wm" name="inv_ixm42xxx_configure_fifo_wm">
<area shape="rect" id="node1" title="Configure Fifo watermark (also refered to as fifo threshold)" alt="" coords="5,129,164,171"/>
<area shape="rect" id="node2" href="$group___driver_ixm42xxx_driver___h_l.html#ga66c5185abd16d812763091b79a678616" title="Retrieve interrupts configuration." alt="" coords="216,137,403,163"/>
<area shape="rect" id="node5" href="$group___driver_ixm42xxx_transport.html#ga1ff0b8e2eb26c611b82e795b6653ff1a" title="Writes data to a register on Ixm42xxx." alt="" coords="688,187,847,214"/>
<area shape="rect" id="node6" href="$group___driver_ixm42xxx_driver___h_l.html#ga01d140f0c4cdd75e519b40c37f520a6b" title="Retrieve interrupts configuration." alt="" coords="212,187,407,214"/>
<area shape="rect" id="node7" href="$group___driver_ixm42xxx_driver___h_l.html#ga02d9e73649adc7063b87b528789da746" title="Retrieve interrupts configuration." alt="" coords="212,86,407,113"/>
<area shape="rect" id="node8" href="$group___driver_ixm42xxx_driver___h_l.html#gaffb6e096b26cce389121a6fcd33ad546" title="Configure which interrupt source can trigger ibi interruptions." alt="" coords="216,289,403,315"/>
<area shape="rect" id="node9" href="$group___driver_ixm42xxx_driver___h_l.html#ga14aafe11842b6f9df47e4ebe56334db9" title="Configure which interrupt source can trigger INT1." alt="" coords="212,35,407,62"/>
<area shape="rect" id="node10" href="$group___driver_ixm42xxx_driver___h_l.html#gaf17db67a06978d2e94dfff9684c513fe" title="Configure which interrupt source can trigger INT2." alt="" coords="212,238,407,265"/>
<area shape="rect" id="node3" href="$group___driver_ixm42xxx_transport.html#ga649560d180b5c0018269d3a83597acc6" title="Reads data from a register on Ixm42xxx." alt="" coords="469,137,626,163"/>
<area shape="rect" id="node4" href="$group___driver_ixm42xxx_driver___h_l.html#ga8817386c1e4b5d4ee66238e2c6172f09" title="Set register bank index." alt="" coords="455,187,640,214"/>
</map>
