| eMD IIM4265x Driver API 1.0.0

Data Structures | Data Fields
inv_ixm42xxx_transport Struct Reference
Ixm42xxx driver transport

transport interface More...

`#include <Ixm42xxxTransport.h>`

Collaboration diagram for inv_ixm42xxx_transport:
[legend]

## Data Structures
struct | register_cache
| Contains mirrored values of some IP registers. More...

## Data Fields
struct inv_ixm42xxx_serif | serif
struct inv_ixm42xxx_transport::register_cache | register_cache

## Detailed Description

transport interface

Definition at line 73 of file Ixm42xxxTransport.h.

## Field Documentation

## ◆ register_cache

struct inv_ixm42xxx_transport::register_cache register_cache

Store mostly used register values on SRAM. MPUREG_OTP_SEC_STATUS_B1 and MPUREG_INT_STATUS registers are read before the cache has a chance to be initialized. Therefore, these registers shall never be added to the cache Registers from bank 1,2,3 or 4 shall never be added to the cache

## ◆ serif

struct inv_ixm42xxx_serif serif

Warning : this field MUST be the first one of struct inv_ixm42xxx_transport

Definition at line 68 of file Ixm42xxxTransport.h.

The documentation for this struct was generated from the following file:

- Ixm42xxxTransport.h