| eMD IIM4265x Driver API 1.0.0

Data Fields
inv_ixm42xxx_tap_parameters_t Struct Reference
Ixm42xxx driver high level functions related to APEX

Ixm42xxx TAP inputs parameters definition. More...

`#include <Ixm42xxxDriver_HL_apex.h>`

## Data Fields
uint8_t | min_jerk_thr
IXM42XXX_APEX_CONFIG7_TAP_MAX_PEAK_TOL_t | max_peak_tol
IXM42XXX_APEX_CONFIG8_TAP_TMAX_t | tmax
IXM42XXX_APEX_CONFIG8_TAP_TAVG_t | tavg
IXM42XXX_APEX_CONFIG8_TAP_TMIN_t | tmin

## Detailed Description

Ixm42xxx TAP inputs parameters definition.

Definition at line 53 of file Ixm42xxxDriver_HL_apex.h.

## Field Documentation

## ◆ max_peak_tol

IXM42XXX_APEX_CONFIG7_TAP_MAX_PEAK_TOL_t max_peak_tol

Maximum peak tolerance

Definition at line 55 of file Ixm42xxxDriver_HL_apex.h.

## ◆ min_jerk_thr

uint8_t min_jerk_thr

Minimum Jerk Threshold

Definition at line 54 of file Ixm42xxxDriver_HL_apex.h.

## ◆ tavg

IXM42XXX_APEX_CONFIG8_TAP_TAVG_t tavg

Energy measumerement window

Definition at line 57 of file Ixm42xxxDriver_HL_apex.h.

## ◆ tmax

IXM42XXX_APEX_CONFIG8_TAP_TMAX_t tmax

Tap measurement window

Definition at line 56 of file Ixm42xxxDriver_HL_apex.h.

## ◆ tmin

IXM42XXX_APEX_CONFIG8_TAP_TMIN_t tmin

Single tap window

Definition at line 58 of file Ixm42xxxDriver_HL_apex.h.

The documentation for this struct was generated from the following file:

- Ixm42xxxDriver_HL_apex.h