<map id="inv_ixm42xxx_disable_gyro" name="inv_ixm42xxx_disable_gyro">
<area shape="rect" id="node1" title="Disable all 3 axes of gyro." alt="" coords="5,181,185,207"/>
<area shape="rect" id="node2" href="$group___driver_ixm42xxx_driver___h_l.html#ga21e1b725b1c8d8fe36f896c831f883bd" title="Converts IXM42XXX_ACCEL_CONFIG0_ODR_t or IXM42XXX_GYRO_CONFIG0_ODR_t enums to period expressed in us." alt="" coords="249,5,397,47"/>
<area shape="rect" id="node3" href="$group___driver_ixm42xxx_driver___h_l.html#gac62cde6e351bbc64c80183882fec8652" title="Configure Accel clock source." alt="" coords="255,173,390,215"/>
<area shape="rect" id="node4" href="$group___driver_ixm42xxx_transport.html#ga649560d180b5c0018269d3a83597acc6" title="Reads data from a register on Ixm42xxx." alt="" coords="461,122,618,149"/>
<area shape="rect" id="node5" href="$group___driver_ixm42xxx_transport.html#ga1ff0b8e2eb26c611b82e795b6653ff1a" title="Writes data to a register on Ixm42xxx." alt="" coords="460,181,619,207"/>
<area shape="rect" id="node6" href="$group___driver_ixm42xxx_ext.html#gaeb9882b24403dcf897e8f3ce1d701651" title="Hook for low&#45;level high res system get_time() function to be implemented by upper layer Timer should ..." alt="" coords="233,290,412,317"/>
<area shape="rect" id="node7" href="$group___driver_ixm42xxx_driver___h_l.html#ga978d6a926ad4124c331c0463aeb15145" title="reset IXM42XXX fifo" alt="" coords="243,122,402,149"/>
<area shape="rect" id="node8" href="$group___driver_ixm42xxx_ext.html#gac7b05db7fc2dcb42a571144e94a6355d" title="Hook for low&#45;level high res system sleep() function to be implemented by upper layer ~100us resolutio..." alt="" coords="243,341,402,367"/>
</map>
