| eMD IIM4265x Driver API 1.0.0

Data Fields
fifo_header_t Union Reference

`#include <Ixm42xxxDefs.h>`

## Data Fields
unsigned char | Byte
struct {
unsigned char gyro_odr_different: 1
unsigned char accel_odr_different: 1
unsigned char fsync_bit: 1
unsigned char timestamp_bit: 1
unsigned char twentybits_bit: 1
unsigned char gyro_bit: 1
unsigned char accel_bit: 1
unsigned char msg_bit: 1
} | bits

## Detailed Description

Describe the content of the FIFO header

Definition at line 241 of file Ixm42xxxDefs.h.

## Field Documentation

## ◆ accel_bit

unsigned char accel_bit

Definition at line 252 of file Ixm42xxxDefs.h.

## ◆ accel_odr_different

unsigned char accel_odr_different

Definition at line 247 of file Ixm42xxxDefs.h.

## ◆ bits

struct { ... } bits

## ◆ Byte

unsigned char Byte

Definition at line 243 of file Ixm42xxxDefs.h.

## ◆ fsync_bit

unsigned char fsync_bit

Definition at line 248 of file Ixm42xxxDefs.h.

## ◆ gyro_bit

unsigned char gyro_bit

Definition at line 251 of file Ixm42xxxDefs.h.

## ◆ gyro_odr_different

unsigned char gyro_odr_different

Definition at line 246 of file Ixm42xxxDefs.h.

## ◆ msg_bit

unsigned char msg_bit

Definition at line 253 of file Ixm42xxxDefs.h.

## ◆ timestamp_bit

unsigned char timestamp_bit

Definition at line 249 of file Ixm42xxxDefs.h.

## ◆ twentybits_bit

unsigned char twentybits_bit

Definition at line 250 of file Ixm42xxxDefs.h.

The documentation for this union was generated from the following file:

- Ixm42xxxDefs.h