| eMD IIM4265x Driver API 1.0.0

Data Fields
inv_ixm42xxx_tap_data Struct Reference
Ixm42xxx driver high level functions related to APEX

TAP outputs. More...

`#include <Ixm42xxxDriver_HL_apex.h>`

## Data Fields
IXM42XXX_APEX_DATA4_TAP_NUM_t | tap_num
IXM42XXX_APEX_DATA4_TAP_AXIS_t | tap_axis
IXM42XXX_APEX_DATA4_TAP_DIR_t | tap_dir
uint8_t | double_tap_timing

## Detailed Description

TAP outputs.

Definition at line 102 of file Ixm42xxxDriver_HL_apex.h.

## Field Documentation

## ◆ double_tap_timing

uint8_t double_tap_timing

Timing between both taps of a double tap expressed in 1/16th of odr in ms (e.g At 500Hz, 2 means 64ms between each tap)

Definition at line 106 of file Ixm42xxxDriver_HL_apex.h.

## ◆ tap_axis

IXM42XXX_APEX_DATA4_TAP_AXIS_t tap_axis

Axis along which tap has been detected

Definition at line 104 of file Ixm42xxxDriver_HL_apex.h.

## ◆ tap_dir

IXM42XXX_APEX_DATA4_TAP_DIR_t tap_dir

Direction of the tap, either +axis (1) or -axis (0)

Definition at line 105 of file Ixm42xxxDriver_HL_apex.h.

## ◆ tap_num

IXM42XXX_APEX_DATA4_TAP_NUM_t tap_num

Detects single (1) or double (2) tap

Definition at line 103 of file Ixm42xxxDriver_HL_apex.h.

The documentation for this struct was generated from the following file:

- Ixm42xxxDriver_HL_apex.h