<map id="inv_ixm42xxx_enable_accel_low_noise_mode" name="inv_ixm42xxx_enable_accel_low_noise_mode">
<area shape="rect" id="node1" title="Enable/put accel in low noise mode." alt="" coords="5,152,168,193"/>
<area shape="rect" id="node2" href="$group___driver_ixm42xxx_driver___h_l.html#ga21e1b725b1c8d8fe36f896c831f883bd" title="Converts IXM42XXX_ACCEL_CONFIG0_ODR_t or IXM42XXX_GYRO_CONFIG0_ODR_t enums to period expressed in us." alt="" coords="231,5,379,47"/>
<area shape="rect" id="node3" href="$group___driver_ixm42xxx_driver___h_l.html#gac62cde6e351bbc64c80183882fec8652" title="Configure Accel clock source." alt="" coords="238,123,373,164"/>
<area shape="rect" id="node4" href="$group___driver_ixm42xxx_transport.html#ga649560d180b5c0018269d3a83597acc6" title="Reads data from a register on Ixm42xxx." alt="" coords="443,103,601,130"/>
<area shape="rect" id="node5" href="$group___driver_ixm42xxx_transport.html#ga1ff0b8e2eb26c611b82e795b6653ff1a" title="Writes data to a register on Ixm42xxx." alt="" coords="443,158,601,185"/>
<area shape="rect" id="node6" href="$group___driver_ixm42xxx_ext.html#gaeb9882b24403dcf897e8f3ce1d701651" title="Hook for low&#45;level high res system get_time() function to be implemented by upper layer Timer should ..." alt="" coords="216,239,395,266"/>
<area shape="rect" id="node7" href="$group___driver_ixm42xxx_ext.html#gac7b05db7fc2dcb42a571144e94a6355d" title="Hook for low&#45;level high res system sleep() function to be implemented by upper layer ~100us resolutio..." alt="" coords="226,290,385,317"/>
</map>
