| eMD IIM4265x Driver API 1.0.0

Data Fields
inv_ixm42xxx_sensor_event_t Struct Reference
Ixm42xxx driver high level functions

Sensor event structure definition. More...

`#include <Ixm42xxxDriver_HL.h>`

## Data Fields
int | sensor_mask
uint16_t | timestamp_fsync
int16_t | accel [3]
int16_t | gyro [3]
int16_t | temperature
int8_t | accel_high_res [3]
int8_t | gyro_high_res [3]

## Detailed Description

Sensor event structure definition.

Definition at line 152 of file Ixm42xxxDriver_HL.h.

## Field Documentation

## ◆ accel

int16_t accel[3]

Definition at line 155 of file Ixm42xxxDriver_HL.h.

## ◆ accel_high_res

int8_t accel_high_res[3]

Definition at line 158 of file Ixm42xxxDriver_HL.h.

## ◆ gyro

int16_t gyro[3]

Definition at line 156 of file Ixm42xxxDriver_HL.h.

## ◆ gyro_high_res

int8_t gyro_high_res[3]

Definition at line 159 of file Ixm42xxxDriver_HL.h.

## ◆ sensor_mask

int sensor_mask

Definition at line 153 of file Ixm42xxxDriver_HL.h.

## ◆ temperature

int16_t temperature

Definition at line 157 of file Ixm42xxxDriver_HL.h.

## ◆ timestamp_fsync

uint16_t timestamp_fsync

Definition at line 154 of file Ixm42xxxDriver_HL.h.

The documentation for this struct was generated from the following file:

- Ixm42xxxDriver_HL.h