| ICM45605 eMD driver Documentation of the eMD Driver API

- Main Page
- Related Pages
- Modules
- Classes
- Files

- Class List
- Class Index
- Class Members

Public Attributes | List of all members
inv_imu_edmp_int_state_t Struct Reference
EDMP

APEX interrupts definition. More...

`#include <inv_imu_edmp.h>`

## Public Attributes
uint8_t | INV_TAP
uint8_t | INV_HIGHG
uint8_t | INV_LOWG
uint8_t | INV_TILT_DET
uint8_t | INV_STEP_CNT_OVFL
uint8_t | INV_STEP_DET
uint8_t | INV_FF
uint8_t | INV_R2W
uint8_t | INV_B2S
uint8_t | INV_R2W_SLEEP
uint8_t | INV_B2S_REV
uint8_t | INV_SMD
uint8_t | INV_SELF_TEST
uint8_t | INV_SEC_AUTH

## Detailed Description

APEX interrupts definition.

## Member Data Documentation

## ◆ INV_B2S

uint8_t inv_imu_edmp_int_state_t::INV_B2S

## ◆ INV_B2S_REV

uint8_t inv_imu_edmp_int_state_t::INV_B2S_REV

## ◆ INV_FF

uint8_t inv_imu_edmp_int_state_t::INV_FF

## ◆ INV_HIGHG

uint8_t inv_imu_edmp_int_state_t::INV_HIGHG

## ◆ INV_LOWG

uint8_t inv_imu_edmp_int_state_t::INV_LOWG

## ◆ INV_R2W

uint8_t inv_imu_edmp_int_state_t::INV_R2W

## ◆ INV_R2W_SLEEP

uint8_t inv_imu_edmp_int_state_t::INV_R2W_SLEEP

## ◆ INV_SEC_AUTH

uint8_t inv_imu_edmp_int_state_t::INV_SEC_AUTH

## ◆ INV_SELF_TEST

uint8_t inv_imu_edmp_int_state_t::INV_SELF_TEST

## ◆ INV_SMD

uint8_t inv_imu_edmp_int_state_t::INV_SMD

## ◆ INV_STEP_CNT_OVFL

uint8_t inv_imu_edmp_int_state_t::INV_STEP_CNT_OVFL

## ◆ INV_STEP_DET

uint8_t inv_imu_edmp_int_state_t::INV_STEP_DET

## ◆ INV_TAP

uint8_t inv_imu_edmp_int_state_t::INV_TAP

## ◆ INV_TILT_DET

uint8_t inv_imu_edmp_int_state_t::INV_TILT_DET

The documentation for this struct was generated from the following file:

- inv_imu_edmp.h