| DK45605 eMD examples User Guide 2.1.0 Documentation of the DK45605 eMD examples

- Main Page
- Related Pages

basic_read_fifo

This application demonstrates how to retrieve data from the FIFO using the basic driver. FIFO threshold is set to 1 packet and configured on INT1. Accel and gyro ODR are set to 50 Hz.

# Command interface

This application allows the following command to be sent through UART:

- `s`: to toggle print data in SI unit (defaults to enable).
- `l`: to toggle print data in LSB (defaults to disable).
- `a`: to toggle enable/disable accelerometer (defaults to enable).
- `g`: to toggle enable/disable gyroscope (defaults to enable).
- `i`: to toggle enable/disable FIFO high-resolution mode (defaults to disable).
- `p`: to select low-noise or low-power sensor mode, common to accelerometer and gyroscope (defaults to low-noise).
- `c`: to print current configuration.
- `h`: to print help screen.

# Terminal output

## Data format

Data are printed on the terminal as follow:

- When print in SI unit is enabled:
  SI <timestamp> us Accel: <acc_x> <acc_y> <acc_z> g Gyro: <gyr_x> <gyr_y> <gyr_z> dps Temp: <temp> degC FIFO time: <fifo_time> us
- When print in LSB is enabled:
  LSB <timestamp> us Accel: <raw_acc_x> <raw_acc_y> <raw_acc_z> Gyro: <raw_gyr_x> <raw_gyr_y> <raw_gyr_z> Temp: <raw_temp> FIFO time: <fifo_time> us

With:

- `<timestamp>`: Time in microsecond read from MCU clock when latest INT1 was fired
- `<raw_acc_x|y|z>`: Raw accelerometer value
- `<acc_x|y|z>`: Raw accelerometer value converted in g
- `<raw_gyr_x|y|z>`: Raw gyroscope value
- `<gyr_x|y|z>`: Raw gyroscope value converted in dps
- `<raw_temp>`: Raw temperature value
- `<temp>`: Raw temperature value converted in °C
- `<fifo_time>`: 16-bit timestamp field in us as read in FIFO, this is time at which ICM samples current FIFO packet, unit being 1 us or 16 us depending on ICM configuration (defaults to 1 us). Rolls over 65535.

## Example of output

[I] ###
[I] ### Example Read FIFO (using basic API)
[I] ###
[I] SI 7262 us Accel: -0.02 0.01 1.01 g Gyro: - - - Temp: 27.00 degC FIFO Time: 1718 us
[I] SI 27162 us Accel: -0.02 0.01 1.01 g Gyro: -2.32 0.12 0.37 dps Temp: 27.50 degC FIFO Time: 21718 us
[I] SI 47045 us Accel: -0.02 0.01 1.01 g Gyro: -2.32 0.06 0.24 dps Temp: 27.50 degC FIFO Time: 41718 us
[I] SI 66929 us Accel: -0.02 0.01 1.01 g Gyro: -2.32 -0.06 0.06 dps Temp: 27.50 degC FIFO Time: 61718 us
[I] SI 86813 us Accel: -0.02 0.01 1.01 g Gyro: -2.32 -0.06 0.12 dps Temp: 27.00 degC FIFO Time: 16182 us
[I] SI 106696 us Accel: -0.02 0.01 1.01 g Gyro: -2.32 0.00 0.12 dps Temp: 27.00 degC FIFO Time: 36182 us
[I] SI 126580 us Accel: -0.02 0.01 1.01 g Gyro: -2.32 -0.06 0.12 dps Temp: 27.00 degC FIFO Time: 56182 us
[I] SI 146463 us Accel: -0.02 0.01 1.01 g Gyro: -2.32 0.00 0.12 dps Temp: 27.50 degC FIFO Time: 10646 us
[I] SI 166347 us Accel: -0.02 0.01 1.01 g Gyro: -2.32 0.00 0.12 dps Temp: 27.50 degC FIFO Time: 30646 us
[I] SI 186231 us Accel: -0.02 0.01 1.01 g Gyro: -2.32 0.00 0.18 dps Temp: 27.00 degC FIFO Time: 50646 us
[I] SI 206114 us Accel: -0.02 0.01 1.01 g Gyro: -2.26 0.00 0.12 dps Temp: 27.50 degC FIFO Time: 5110 us
[I] SI 225998 us Accel: -0.02 0.01 1.01 g Gyro: -2.32 0.00 0.12 dps Temp: 27.00 degC FIFO Time: 25110 us
[I] SI 245881 us Accel: -0.02 0.01 1.01 g Gyro: -2.32 0.00 0.12 dps Temp: 27.50 degC FIFO Time: 45110 us
[I] SI 265765 us Accel: -0.02 0.01 1.01 g Gyro: -2.32 0.00 0.12 dps Temp: 27.50 degC FIFO Time: 65110 us
[I] SI 285649 us Accel: -0.02 0.01 1.01 g Gyro: -2.32 0.00 0.12 dps Temp: 27.50 degC FIFO Time: 19574 us
[I] SI 305532 us Accel: -0.02 0.01 1.01 g Gyro: -2.32 -0.06 0.06 dps Temp: 27.50 degC FIFO Time: 39574 us
[I] Disabling SI print.
[I] Enabling LSB print.
[I] LSB 1916104 us Accel: -168 57 8299 Gyro: -38 0 2 Temp: 5 FIFO Time: 21174 us
[I] LSB 1935988 us Accel: -163 57 8305 Gyro: -38 0 2 Temp: 4 FIFO Time: 41174 us
[I] LSB 1955871 us Accel: -165 54 8301 Gyro: -38 -2 2 Temp: 5 FIFO Time: 61174 us
[I] LSB 1975755 us Accel: -165 56 8298 Gyro: -38 1 2 Temp: 4 FIFO Time: 15638 us
[I] LSB 1995639 us Accel: -171 52 8303 Gyro: -38 1 2 Temp: 5 FIFO Time: 35638 us
[I] LSB 2015522 us Accel: -178 50 8304 Gyro: -38 0 2 Temp: 4 FIFO Time: 55638 us
[I] LSB 2035406 us Accel: -176 49 8303 Gyro: -38 1 2 Temp: 4 FIFO Time: 10102 us
[I] LSB 2055290 us Accel: -173 52 8304 Gyro: -38 -1 2 Temp: 5 FIFO Time: 30102 us
[I] LSB 2075173 us Accel: -171 58 8302 Gyro: -38 -2 2 Temp: 5 FIFO Time: 50102 us
[I] LSB 2095057 us Accel: -166 56 8301 Gyro: -38 0 2 Temp: 5 FIFO Time: 4566 us
[I] LSB 2114940 us Accel: -168 49 8306 Gyro: -38 0 2 Temp: 5 FIFO Time: 24566 us
[I] LSB 2134824 us Accel: -175 50 8305 Gyro: -37 -1 2 Temp: 4 FIFO Time: 44566 us