| ICM45605 eMD driver Documentation of the eMD Driver API

- Main Page
- Related Pages
- Modules
- Classes
- Files

- Class List
- Class Index
- Class Members

- All
- Variables

- a
- b
- c
- d
- e
- f
- g
- h
- i
- l
- n
- o
- p
- r
- s
- t
- u
- v
- w

Here is a list of all class members with links to the classes they belong to:

### - i -

- i2cm_busy : i2cm_status_t
- i2cm_done : i2cm_status_t
- i2cm_ext_dev_status : i2cm_ext_dev_status_t
- i2cm_go : i2cm_control_t
- i2cm_rd_data0 : i2cm_rd_data0_t
- i2cm_rd_data1 : i2cm_rd_data1_t
- i2cm_rd_data10 : i2cm_rd_data10_t
- i2cm_rd_data11 : i2cm_rd_data11_t
- i2cm_rd_data12 : i2cm_rd_data12_t
- i2cm_rd_data13 : i2cm_rd_data13_t
- i2cm_rd_data14 : i2cm_rd_data14_t
- i2cm_rd_data15 : i2cm_rd_data15_t
- i2cm_rd_data16 : i2cm_rd_data16_t
- i2cm_rd_data17 : i2cm_rd_data17_t
- i2cm_rd_data18 : i2cm_rd_data18_t
- i2cm_rd_data19 : i2cm_rd_data19_t
- i2cm_rd_data2 : i2cm_rd_data2_t
- i2cm_rd_data20 : i2cm_rd_data20_t
- i2cm_rd_data3 : i2cm_rd_data3_t
- i2cm_rd_data4 : i2cm_rd_data4_t
- i2cm_rd_data5 : i2cm_rd_data5_t
- i2cm_rd_data6 : i2cm_rd_data6_t
- i2cm_rd_data7 : i2cm_rd_data7_t
- i2cm_rd_data8 : i2cm_rd_data8_t
- i2cm_rd_data9 : i2cm_rd_data9_t
- i2cm_restart_en : i2cm_control_t
- i2cm_scl_err : i2cm_status_t
- i2cm_sda_err : i2cm_status_t
- i2cm_speed : i2cm_control_t
- i2cm_srst_err : i2cm_status_t
- i2cm_timeout_err : i2cm_status_t
- i2cm_wr_data0 : i2cm_wr_data0_t
- i2cm_wr_data1 : i2cm_wr_data1_t
- i2cm_wr_data2 : i2cm_wr_data2_t
- i2cm_wr_data3 : i2cm_wr_data3_t
- i2cm_wr_data4 : i2cm_wr_data4_t
- i2cm_wr_data5 : i2cm_wr_data5_t
- i3c_stc_mode : sifs_i3c_stc_cfg_t
- init_en : edmp_apex_en1_t
- int0_tdeassert_disable : int_pulse_min_off_intf0_t
- int0_tpulse_duration : int_pulse_min_on_intf0_t
- int1_config0 : intx_configx_t
- int1_config1 : intx_configx_t
- int1_drive : int1_config2_t
- int1_mode : int1_config2_t
- int1_polarity : int1_config2_t
- int1_status0 : intx_statusx_t
- int1_status1 : intx_statusx_t
- int1_status_ap_agc_rdy : int1_status0_t
- int1_status_ap_fsync : int1_status0_t
- int1_status_apex_event : int1_status1_t
- int1_status_aux1_agc_rdy : int1_status0_t
- int1_status_aux1_drdy : int1_status0_t
- int1_status_drdy : int1_status0_t
- int1_status_en_ap_agc_rdy : int1_config0_t
- int1_status_en_ap_fsync : int1_config0_t
- int1_status_en_apex_event : int1_config1_t
- int1_status_en_aux1_agc_rdy : int1_config0_t
- int1_status_en_aux1_drdy : int1_config0_t
- int1_status_en_drdy : int1_config0_t
- int1_status_en_fifo_full : int1_config0_t
- int1_status_en_fifo_ths : int1_config0_t
- int1_status_en_i2cm_done : int1_config1_t
- int1_status_en_i3c_protocol_err : int1_config1_t
- int1_status_en_pll_rdy : int1_config1_t
- int1_status_en_reset_done : int1_config0_t
- int1_status_en_wom_x : int1_config1_t
- int1_status_en_wom_y : int1_config1_t
- int1_status_en_wom_z : int1_config1_t
- int1_status_fifo_full : int1_status0_t
- int1_status_fifo_ths : int1_status0_t
- int1_status_i2cm_done : int1_status1_t
- int1_status_i3c_protocol_err : int1_status1_t
- int1_status_pll_rdy : int1_status1_t
- int1_status_reset_done : int1_status0_t
- int1_status_wom_x : int1_status1_t
- int1_status_wom_y : int1_status1_t
- int1_status_wom_z : int1_status1_t
- int1_tdeassert_disable : int_pulse_min_off_intf1_t
- int1_tpulse_duration : int_pulse_min_on_intf1_t
- int2_drive : int2_config2_t
- int2_mode : int2_config2_t
- int2_polarity : int2_config2_t
- int2_status_ap_agc_rdy : int2_status0_t
- int2_status_ap_fsync : int2_status0_t
- int2_status_apex_event : int2_status1_t
- int2_status_aux1_agc_rdy : int2_status0_t
- int2_status_aux1_drdy : int2_status0_t
- int2_status_drdy : int2_status0_t
- int2_status_en_ap_agc_rdy : int2_config0_t
- int2_status_en_ap_fsync : int2_config0_t
- int2_status_en_apex_event : int2_config1_t
- int2_status_en_aux1_agc_rdy : int2_config0_t
- int2_status_en_aux1_drdy : int2_config0_t
- int2_status_en_drdy : int2_config0_t
- int2_status_en_fifo_full : int2_config0_t
- int2_status_en_fifo_ths : int2_config0_t
- int2_status_en_i2cm_done : int2_config1_t
- int2_status_en_i3c_protocol_err : int2_config1_t
- int2_status_en_pll_rdy : int2_config1_t
- int2_status_en_reset_done : int2_config0_t
- int2_status_en_wom_x : int2_config1_t
- int2_status_en_wom_y : int2_config1_t
- int2_status_en_wom_z : int2_config1_t
- int2_status_fifo_full : int2_status0_t
- int2_status_fifo_ths : int2_status0_t
- int2_status_i2cm_done : int2_status1_t
- int2_status_i3c_protocol_err : int2_status1_t
- int2_status_pll_rdy : int2_status1_t
- int2_status_reset_done : int2_status0_t
- int2_status_wom_x : int2_status1_t
- int2_status_wom_y : int2_status1_t
- int2_status_wom_z : int2_status1_t
- int_accel_drdy_pin_0_dis : status_mask_pin_0_7_t
- int_accel_drdy_pin_1_dis : status_mask_pin_8_15_t
- int_accel_drdy_pin_2_dis : status_mask_pin_16_23_t
- int_apex_config0 : int_apex_configx_t
- int_apex_config1 : int_apex_configx_t
- int_apex_status0 : int_apex_statusx_t
- int_apex_status1 : int_apex_statusx_t
- int_drive : inv_imu_int_pin_config_t
- int_en_aux2_agc_rdy : int_aux2_config_t
- int_en_aux2_drdy : int_aux2_config_t
- int_en_aux2_pll_rdy : int_aux2_config_t
- int_en_aux2_reset_done : int_aux2_config_t
- int_ext_odr_drdy_pin_0_dis : status_mask_pin_0_7_t
- int_ext_odr_drdy_pin_1_dis : status_mask_pin_8_15_t
- int_ext_odr_drdy_pin_2_dis : status_mask_pin_16_23_t
- int_mode : inv_imu_int_pin_config_t
- int_on_demand_pin_0_dis : status_mask_pin_0_7_t
- int_on_demand_pin_1_dis : status_mask_pin_8_15_t
- int_on_demand_pin_2_dis : status_mask_pin_16_23_t
- int_polarity : inv_imu_int_pin_config_t
- int_status_accel_drdy_pin_0 : isr_0_7_t
- int_status_accel_drdy_pin_1 : isr_8_15_t
- int_status_accel_drdy_pin_2 : isr_16_23_t
- int_status_aux2_agc_rdy : int_aux2_status_t
- int_status_aux2_drdy : int_aux2_status_t
- int_status_aux2_pll_rdy : int_aux2_status_t
- int_status_aux2_reset_done : int_aux2_status_t
- int_status_basic_smd : int_apex_status1_t
- int_status_ext_odr_drdy_pin_0 : isr_0_7_t
- int_status_ext_odr_drdy_pin_1 : isr_8_15_t
- int_status_ext_odr_drdy_pin_2 : isr_16_23_t
- int_status_ff_det : int_apex_status0_t
- int_status_high_g_det : int_apex_status0_t
- int_status_i2cm_ioc_ext_trig_en : int_i2cm_source_t
- int_status_i2cm_smc_ext_odr_en : int_i2cm_source_t
- int_status_low_g_det : int_apex_status0_t
- int_status_mask_pin_basic_smd : int_apex_config1_t
- int_status_mask_pin_ff_det : int_apex_config0_t
- int_status_mask_pin_high_g_det : int_apex_config0_t
- int_status_mask_pin_low_g_det : int_apex_config0_t
- int_status_mask_pin_r2w_sleep_det : int_apex_config1_t
- int_status_mask_pin_r2w_wake_det : int_apex_config0_t
- int_status_mask_pin_sa_done : int_apex_config1_t
- int_status_mask_pin_selftest_done : int_apex_config1_t
- int_status_mask_pin_smd_det : int_apex_config1_t
- int_status_mask_pin_step_cnt_ovfl : int_apex_config0_t
- int_status_mask_pin_step_det : int_apex_config0_t
- int_status_mask_pin_tap_detect : int_apex_config0_t
- int_status_mask_pin_tilt_det : int_apex_config0_t
- int_status_on_demand_pin_0 : isr_0_7_t
- int_status_on_demand_pin_1 : isr_8_15_t
- int_status_on_demand_pin_2 : isr_16_23_t
- int_status_r2w_sleep_det : int_apex_status1_t
- int_status_r2w_wake_det : int_apex_status0_t
- int_status_sa_done : int_apex_status1_t
- int_status_selftest_done : int_apex_status1_t
- int_status_smd_det : int_apex_status1_t
- int_status_step_cnt_ovfl : int_apex_status0_t
- int_status_step_det : int_apex_status0_t
- int_status_tap_det : int_apex_status0_t
- int_status_tilt_det : int_apex_status0_t
- INV_AGC_RDY : inv_imu_int_state_t
- INV_B2S : inv_imu_edmp_int_state_t
- INV_B2S_REV : inv_imu_edmp_int_state_t
- INV_EDMP_EVENT : inv_imu_int_state_t
- INV_FF : inv_imu_edmp_int_state_t
- INV_FIFO_FULL : inv_imu_int_state_t
- INV_FIFO_THS : inv_imu_int_state_t
- INV_HIGHG : inv_imu_edmp_int_state_t
- INV_I2CM_DONE : inv_imu_int_state_t
- INV_I3C_PROT_ERR : inv_imu_int_state_t
- INV_LOWG : inv_imu_edmp_int_state_t
- INV_OIS1 : inv_imu_int_state_t
- INV_OIS1_AGC_RDY : inv_imu_int_state_t
- INV_PLL_RDY : inv_imu_int_state_t
- INV_R2W : inv_imu_edmp_int_state_t
- INV_R2W_SLEEP : inv_imu_edmp_int_state_t
- INV_RESET_DONE : inv_imu_int_state_t
- INV_SEC_AUTH : inv_imu_edmp_int_state_t
- INV_SELF_TEST : inv_imu_edmp_int_state_t
- INV_SMD : inv_imu_edmp_int_state_t
- INV_STEP_CNT_OVFL : inv_imu_edmp_int_state_t
- INV_STEP_DET : inv_imu_edmp_int_state_t
- INV_TAP : inv_imu_edmp_int_state_t
- INV_TILT_DET : inv_imu_edmp_int_state_t
- INV_UI_DRDY : inv_imu_int_state_t
- INV_UI_FSYNC : inv_imu_int_state_t
- INV_WOM_X : inv_imu_int_state_t
- INV_WOM_Y : inv_imu_int_state_t
- INV_WOM_Z : inv_imu_int_state_t
- io_opt0 : ipreg_bar_reg_57_t
- io_opt1 : ipreg_bar_reg_57_t
- io_opt2 : ipreg_bar_reg_58_t
- ireg_addr_15_8 : ireg_addr_15_8_t
- ireg_addr_7_0 : ireg_addr_7_0_t
- ireg_data : ireg_data_t
- ireg_done : reg_misc2_t