| ICM45605 eMD driver Documentation of the eMD Driver API

- Main Page
- Related Pages
- Modules
- Classes
- Files

- Class List
- Class Index
- Class Members

Public Attributes | List of all members
intx_statusx_t Struct Reference
Defs

Registers to retrieve interrupts status. More...

`#include <inv_imu_defs.h>`

Collaboration diagram for intx_statusx_t:
[legend]

## Public Attributes
int1_status0_t | int1_status0
int1_status1_t | int1_status1

## Detailed Description

Registers to retrieve interrupts status.

This structure applies to INT1 and INT2 as bit location are the same.

## Member Data Documentation

## ◆ int1_status0

int1_status0_t intx_statusx_t::int1_status0

## ◆ int1_status1

int1_status1_t intx_statusx_t::int1_status1

The documentation for this struct was generated from the following file:

- inv_imu_defs.h