| DK45605 eMD examples User Guide 2.1.0 Documentation of the DK45605 eMD examples

- Main Page
- Related Pages

Sensorcli

Sensorcli is a command line interface used to receive data and control firmware from a computer when the dynamic protocol is being implemented. Arguments are optional and can be listed with `--help`.

In the context of sensorcli, the word "sensor" designates the various firmware outputs and can represent raw sensor data or algorithm's outputs.

# Commands

The full list of available commands can be retrieved with the `help` command. The following table lists the most useful ones.

Arguments within brackets (`[arg]`) are optional.

Command | Description
--- | ---
`help [command]` | If `command` is not provided, list all available commands. Otherwise, provide details about the requested command.
`ids` | List sensor type to be used in other command (designated by `sensor_name`). Commonly used ids are: `racc` for raw accel `rgyr` for raw gyro `rtemp` for raw temperature `rmag` for raw mag `acc` for calibrated accel `gyr` for calibrated gyro `temp` for calibrated temperature `mag` for calibrated mag `grv` for game rotation vector (6-axis fusion) `rv` for rotation vector (9-axis fusion)
`en sensor_name` | Enable the sensor designated by `sensor_name`
`dis sensor_name` | Disable the sensor designated by `sensor_name`
`ping` | Interrogates firmware and lists all available sensors.
`disp off [sensor_name]` | Stop displaying sensor data. If `sensor_name` is provided, only the specified sensor data will stop being displayed. If no argument is provided, all sensors data will stop being displayed. Note: This doesn't disable sensors, it only stops printing them on the console.
`disp on [sensor_name]` | Start displaying sensor data. If `sensor_name` is provided, only the specified sensor data will start being displayed. If no argument is provided, all sensors data will start being displayed.
`log on [filename]` | Log sensor data to a file. If `filename` is not specified a file named log_yyyy-mm-dd-H-M-S.txt will be created. If `filename` is specified sensor events will be logged to this file, overwriting its content. If `filename` does not exist, it will be created. Note: To log reliably, it is recommended to turn off display of data in the console (`disp off`).
`log off` | Stop logging sensor data and properly close the file.
`cube on sensor_name` | Display a cube whose orientation is based on `sensor_name` data (must be a quaternion). Note: In order for the cube to receive data, `sensor_name` must be enabled using `en sensor_name` command. Tip: Turning off the display of data in the console (`disp off`) might smoothen the movement of the cube.
`cube off sensor_name` | Stop displaying the cube for the specified sensor.
`cube setref sensor_name` | Set the current orientation as reference for the cube for the specified sensor.
`cube resetref sensor_name` | Clear the reference for the cube for the specified sensor.
`setconfig sensor_name settings=value` | Set a certain configuration for the requested sensor. Supported configuration depends on the firmware, please refer to the application documentation for the full list.
`decode sensor_name descriptor` | Tell sensor-cli how to decode a custom sensor event. `descriptor` consists in a string composed of one or more tokens separated by spaces. Tokens must follows the pattern: `[#\|-\|*]{f\|flt\|float\|d\|dbl\|double\|{s\|sint\|int\|u\|uint}[XX][qYY][_t]}[le\|be][[ZZ]\|\@ZZ]` in which: `[ AAA ]` means AAA is optional `{ AAA \| BBB \| ... }` means it's a choice between AAA, BBB, ... `[ AAA \| BBB \| ... ]` means it's an optional choice between AAA, BBB, ... `#` / `*` / `-` means element should not be returned (useful to indicate padding) `f` / `flt` / `float` stands for float (assuming 4 bytes long) `d` / `dbl` / `double` stands for double (assuming 8 bytes long) `sXX` / `sintXX` / `intXX` / `int` stands for signed integer `uXX` / `uintXX` / `uint` stands for unsigned integer `XX` is the integer length in bits and can be 8, 16, 24, 32, 40, 48, 56, 64 (assuming 32 as default) `qYY` designates the fractional part of a fix point integer `le`, `be` indicates endianness used for encoding (assuming LE as default) `[ZZ]` or `\@ZZ` indicates number of elements to consider being coded the same way Integer types can be suffixed with `_t` in order to be compatible with `<stdint.h>` types. Empty descriptor will reset the decoding to default decoder.
`sleep ms` | Pause the main thread for `ms` millisecond.
`quit` or `exit` | Properly exit sensorcli.

# Usage

## Start a log

Scenario: log raw accel, raw gyro and 6-axis fusion output for 1 min.

sensor-cli> disp off; log on my_filename.txt; en racc; en rgyr; en grv; sleep 60000; log off

## Display cube

Scenario: Visualize 6-axis fusion output with the cube.

sensor-cli> disp off; cube on grv; en grv;