| ICM45686 eMD driver Documentation of the eMD Driver API

- Main Page
- Related Pages
- Modules
- Classes
- Files

- Class List
- Class Index
- Class Members

Public Attributes | List of all members
inv_imu_edmp_b2s_parameters_t Struct Reference
EDMP Wearable

IMU B2S parameters definition. More...

`#include <inv_imu_edmp_wearable.h>`

## Public Attributes
uint32_t | b2s_mounting_matrix
| Specifies mounting matrix to be applied to B2S raw data Set bit 2 : swap X/Y ; flip Z Set bit 1 : flip X ; flip Z Set bit 0 : flip Y ; flip Z. More...

## Detailed Description

IMU B2S parameters definition.

## Member Data Documentation

## ◆ b2s_mounting_matrix

uint32_t inv_imu_edmp_b2s_parameters_t::b2s_mounting_matrix

Specifies mounting matrix to be applied to B2S raw data Set bit 2 : swap X/Y ; flip Z Set bit 1 : flip X ; flip Z Set bit 0 : flip Y ; flip Z.

The documentation for this struct was generated from the following file:

- inv_imu_edmp_wearable.h