| ICM45686 eMD driver Documentation of the eMD Driver API

- Main Page
- Related Pages
- Modules
- Classes
- Files

- File List
- File Members

- All
- Functions
- Typedefs
- Enumerations
- Enumerator
- Macros

- a
- d
- e
- f
- g
- i
- o
- p
- r
- s
- t
- u
- w

Here is a list of all file members with links to the files they belong to:

### - i -

- I2CM_COMMAND_0 : inv_imu_regmap_le.h
- I2CM_COMMAND_1 : inv_imu_regmap_le.h
- I2CM_COMMAND_2 : inv_imu_regmap_le.h
- I2CM_COMMAND_3 : inv_imu_regmap_le.h
- I2CM_CONTROL : inv_imu_regmap_le.h
- I2CM_DEV_PROFILE0 : inv_imu_regmap_le.h
- I2CM_DEV_PROFILE1 : inv_imu_regmap_le.h
- I2CM_DEV_PROFILE2 : inv_imu_regmap_le.h
- I2CM_DEV_PROFILE3 : inv_imu_regmap_le.h
- I2CM_EXT_DEV_STATUS : inv_imu_regmap_le.h
- I2CM_RD_DATA0 : inv_imu_regmap_le.h
- I2CM_RD_DATA1 : inv_imu_regmap_le.h
- I2CM_RD_DATA10 : inv_imu_regmap_le.h
- I2CM_RD_DATA11 : inv_imu_regmap_le.h
- I2CM_RD_DATA12 : inv_imu_regmap_le.h
- I2CM_RD_DATA13 : inv_imu_regmap_le.h
- I2CM_RD_DATA14 : inv_imu_regmap_le.h
- I2CM_RD_DATA15 : inv_imu_regmap_le.h
- I2CM_RD_DATA16 : inv_imu_regmap_le.h
- I2CM_RD_DATA17 : inv_imu_regmap_le.h
- I2CM_RD_DATA18 : inv_imu_regmap_le.h
- I2CM_RD_DATA19 : inv_imu_regmap_le.h
- I2CM_RD_DATA2 : inv_imu_regmap_le.h
- I2CM_RD_DATA20 : inv_imu_regmap_le.h
- I2CM_RD_DATA3 : inv_imu_regmap_le.h
- I2CM_RD_DATA4 : inv_imu_regmap_le.h
- I2CM_RD_DATA5 : inv_imu_regmap_le.h
- I2CM_RD_DATA6 : inv_imu_regmap_le.h
- I2CM_RD_DATA7 : inv_imu_regmap_le.h
- I2CM_RD_DATA8 : inv_imu_regmap_le.h
- I2CM_RD_DATA9 : inv_imu_regmap_le.h
- I2CM_STATUS : inv_imu_regmap_le.h
- I2CM_WR_DATA0 : inv_imu_regmap_le.h
- I2CM_WR_DATA1 : inv_imu_regmap_le.h
- I2CM_WR_DATA2 : inv_imu_regmap_le.h
- I2CM_WR_DATA3 : inv_imu_regmap_le.h
- I2CM_WR_DATA4 : inv_imu_regmap_le.h
- I2CM_WR_DATA5 : inv_imu_regmap_le.h
- INT1_CONFIG0 : inv_imu_regmap_le.h
- INT1_CONFIG1 : inv_imu_regmap_le.h
- INT1_CONFIG2 : inv_imu_regmap_le.h
- INT1_STATUS0 : inv_imu_regmap_le.h
- INT1_STATUS1 : inv_imu_regmap_le.h
- INT2_CONFIG0 : inv_imu_regmap_le.h
- INT2_CONFIG1 : inv_imu_regmap_le.h
- INT2_CONFIG2 : inv_imu_regmap_le.h
- INT2_STATUS0 : inv_imu_regmap_le.h
- INT2_STATUS1 : inv_imu_regmap_le.h
- INT4_TO_INT8 : inv_imu_defs.h
- INT5_TO_INT8 : inv_imu_defs.h
- INT_APEX_CONFIG0 : inv_imu_regmap_le.h
- INT_APEX_CONFIG1 : inv_imu_regmap_le.h
- INT_APEX_STATUS0 : inv_imu_regmap_le.h
- INT_APEX_STATUS1 : inv_imu_regmap_le.h
- INT_AUX2_CONFIG : inv_imu_regmap_le.h
- INT_AUX2_STATUS : inv_imu_regmap_le.h
- INT_I2CM_SOURCE : inv_imu_regmap_le.h
- INT_PULSE_MIN_OFF_INTF0 : inv_imu_regmap_le.h
- INT_PULSE_MIN_OFF_INTF1 : inv_imu_regmap_le.h
- INT_PULSE_MIN_ON_INTF0 : inv_imu_regmap_le.h
- INT_PULSE_MIN_ON_INTF1 : inv_imu_regmap_le.h
- INTF_AUX_CONFIG : inv_imu_regmap_le.h
- INTF_CONFIG0 : inv_imu_regmap_le.h
- INTF_CONFIG1_OVRD : inv_imu_regmap_le.h
- INTF_CONFIG1_OVRD_AP_SPI_34_MODE_OVRD_VAL_3_WIRE : inv_imu_defs.h
- INTF_CONFIG1_OVRD_AP_SPI_34_MODE_OVRD_VAL_4_WIRE : inv_imu_defs.h
- intf_config1_ovrd_ap_spi_34_mode_ovrd_val_t : inv_imu_defs.h
- INTF_CONFIG1_OVRD_AP_SPI_MODE_OVRD_VAL_0_OR_3 : inv_imu_defs.h
- INTF_CONFIG1_OVRD_AP_SPI_MODE_OVRD_VAL_1_OR_2 : inv_imu_defs.h
- intf_config1_ovrd_ap_spi_mode_ovrd_val_t : inv_imu_defs.h
- INTF_CONFIG_OVRD_AUX1 : inv_imu_regmap_le.h
- INTF_CONFIG_OVRD_AUX2 : inv_imu_regmap_le.h
- INTX_CONFIG2_INTX_DRIVE_OD : inv_imu_defs.h
- INTX_CONFIG2_INTX_DRIVE_PP : inv_imu_defs.h
- intx_config2_intx_drive_t : inv_imu_defs.h
- INTX_CONFIG2_INTX_MODE_LATCH : inv_imu_defs.h
- INTX_CONFIG2_INTX_MODE_PULSE : inv_imu_defs.h
- intx_config2_intx_mode_t : inv_imu_defs.h
- INTX_CONFIG2_INTX_POLARITY_HIGH : inv_imu_defs.h
- INTX_CONFIG2_INTX_POLARITY_LOW : inv_imu_defs.h
- intx_config2_intx_polarity_t : inv_imu_defs.h
- inv_imu_adv_configure_wom() : inv_imu_driver_advanced.h
- inv_imu_adv_convert_odr_bitfield_to_us() : inv_imu_driver_advanced.h
- inv_imu_adv_device_reset() : inv_imu_driver_advanced.h
- inv_imu_adv_disable_accel() : inv_imu_driver_advanced.h
- inv_imu_adv_disable_gyro() : inv_imu_driver_advanced.h
- inv_imu_adv_disable_wom() : inv_imu_driver_advanced.h
- inv_imu_adv_enable_accel_ln() : inv_imu_driver_advanced.h
- inv_imu_adv_enable_accel_lp() : inv_imu_driver_advanced.h
- inv_imu_adv_enable_gyro_ln() : inv_imu_driver_advanced.h
- inv_imu_adv_enable_gyro_lp() : inv_imu_driver_advanced.h
- inv_imu_adv_enable_wom() : inv_imu_driver_advanced.h
- inv_imu_adv_get_accel_fsr() : inv_imu_driver_advanced.h
- inv_imu_adv_get_data_from_fifo() : inv_imu_driver_advanced.h
- inv_imu_adv_get_data_from_registers() : inv_imu_driver_advanced.h
- inv_imu_adv_get_fifo_config() : inv_imu_driver_advanced.h
- inv_imu_adv_get_gyro_fsr() : inv_imu_driver_advanced.h
- inv_imu_adv_get_timestamp_resolution_us() : inv_imu_driver_advanced.h
- inv_imu_adv_init() : inv_imu_driver_advanced.h
- inv_imu_adv_parse_fifo_data() : inv_imu_driver_advanced.h
- inv_imu_adv_power_down_sram() : inv_imu_driver_advanced.h
- inv_imu_adv_power_up_sram() : inv_imu_driver_advanced.h
- inv_imu_adv_reset_fifo() : inv_imu_driver_advanced.h
- inv_imu_adv_set_endianness() : inv_imu_driver_advanced.h
- inv_imu_adv_set_fifo_config() : inv_imu_driver_advanced.h
- inv_imu_adv_set_timestamp_resolution() : inv_imu_driver_advanced.h
- INV_IMU_DISABLE : inv_imu_defs.h
- inv_imu_edmp_activity_class_t : inv_imu_edmp.h
- inv_imu_edmp_b2s_disable() : inv_imu_edmp_wearable.h
- inv_imu_edmp_b2s_enable() : inv_imu_edmp_wearable.h
- inv_imu_edmp_b2s_get_parameters() : inv_imu_edmp_wearable.h
- inv_imu_edmp_b2s_init() : inv_imu_edmp_wearable.h
- inv_imu_edmp_b2s_set_parameters() : inv_imu_edmp_wearable.h
- inv_imu_edmp_configure() : inv_imu_edmp.h
- inv_imu_edmp_disable() : inv_imu_edmp.h
- inv_imu_edmp_disable_ff() : inv_imu_edmp.h
- inv_imu_edmp_disable_pedometer() : inv_imu_edmp.h
- inv_imu_edmp_disable_r2w() : inv_imu_edmp.h
- inv_imu_edmp_disable_smd() : inv_imu_edmp.h
- inv_imu_edmp_disable_tap() : inv_imu_edmp.h
- inv_imu_edmp_disable_tilt() : inv_imu_edmp.h
- inv_imu_edmp_enable() : inv_imu_edmp.h
- inv_imu_edmp_enable_ff() : inv_imu_edmp.h
- inv_imu_edmp_enable_pedometer() : inv_imu_edmp.h
- inv_imu_edmp_enable_r2w() : inv_imu_edmp.h
- inv_imu_edmp_enable_smd() : inv_imu_edmp.h
- inv_imu_edmp_enable_tap() : inv_imu_edmp.h
- inv_imu_edmp_enable_tilt() : inv_imu_edmp.h
- inv_imu_edmp_get_apex_parameters() : inv_imu_edmp.h
- inv_imu_edmp_get_config_int_apex() : inv_imu_edmp.h
- inv_imu_edmp_get_ff_data() : inv_imu_edmp.h
- inv_imu_edmp_get_int_apex_status() : inv_imu_edmp.h
- inv_imu_edmp_get_pedometer_data() : inv_imu_edmp.h
- inv_imu_edmp_get_tap_data() : inv_imu_edmp.h
- inv_imu_edmp_init_apex() : inv_imu_edmp.h
- INV_IMU_EDMP_INT0 : inv_imu_edmp.h
- INV_IMU_EDMP_INT1 : inv_imu_edmp.h
- INV_IMU_EDMP_INT2 : inv_imu_edmp.h
- inv_imu_edmp_int_t : inv_imu_edmp.h
- inv_imu_edmp_mask_int_src() : inv_imu_edmp.h
- inv_imu_edmp_recompute_apex_decimation() : inv_imu_edmp.h
- INV_IMU_EDMP_RUN : inv_imu_edmp.h
- inv_imu_edmp_run_ondemand() : inv_imu_edmp.h
- inv_imu_edmp_set_apex_parameters() : inv_imu_edmp.h
- inv_imu_edmp_set_config_int_apex() : inv_imu_edmp.h
- inv_imu_edmp_set_frequency() : inv_imu_edmp.h
- inv_imu_edmp_tap_axis_t : inv_imu_edmp.h
- INV_IMU_EDMP_TAP_AXIS_X : inv_imu_edmp.h
- INV_IMU_EDMP_TAP_AXIS_Y : inv_imu_edmp.h
- INV_IMU_EDMP_TAP_AXIS_Z : inv_imu_edmp.h
- INV_IMU_EDMP_TAP_DIR_NEGATIVE : inv_imu_edmp.h
- INV_IMU_EDMP_TAP_DIR_POSITIVE : inv_imu_edmp.h
- inv_imu_edmp_tap_dir_t : inv_imu_edmp.h
- INV_IMU_EDMP_TAP_DOUBLE : inv_imu_edmp.h
- inv_imu_edmp_tap_num_t : inv_imu_edmp.h
- INV_IMU_EDMP_TAP_SINGLE : inv_imu_edmp.h
- INV_IMU_EDMP_UNKNOWN : inv_imu_edmp.h
- inv_imu_edmp_unmask_int_src() : inv_imu_edmp.h
- inv_imu_edmp_wait_for_idle() : inv_imu_edmp.h
- INV_IMU_EDMP_WALK : inv_imu_edmp.h
- INV_IMU_ENABLE : inv_imu_defs.h
- INV_IMU_ERROR : inv_imu_defs.h
- INV_IMU_ERROR_BAD_ARG : inv_imu_defs.h
- INV_IMU_ERROR_EDMP_BUF_EMPTY : inv_imu_defs.h
- INV_IMU_ERROR_EDMP_ODR : inv_imu_defs.h
- INV_IMU_ERROR_TIMEOUT : inv_imu_defs.h
- INV_IMU_ERROR_TRANSPORT : inv_imu_defs.h
- inv_imu_flush_fifo() : inv_imu_driver.h
- inv_imu_get_config_int() : inv_imu_driver.h
- inv_imu_get_endianness() : inv_imu_driver.h
- inv_imu_get_fifo_config() : inv_imu_driver.h
- inv_imu_get_fifo_frame() : inv_imu_driver.h
- inv_imu_get_frame_count() : inv_imu_driver.h
- inv_imu_get_int_status() : inv_imu_driver.h
- inv_imu_get_register_data() : inv_imu_driver.h
- inv_imu_get_version() : inv_imu_driver.h
- inv_imu_get_who_am_i() : inv_imu_driver.h
- INV_IMU_INT1 : inv_imu_defs.h
- INV_IMU_INT2 : inv_imu_defs.h
- inv_imu_int_num_t : inv_imu_defs.h
- INV_IMU_OK : inv_imu_defs.h
- INV_IMU_READ_EDMP_SRAM : inv_imu_edmp.h
- inv_imu_read_reg() : inv_imu_transport.h
- inv_imu_read_reg_t : inv_imu_transport.h
- inv_imu_read_sram() : inv_imu_transport.h
- inv_imu_select_accel_lp_clk() : inv_imu_driver.h
- inv_imu_selftest() : inv_imu_selftest.h
- inv_imu_selftest_init_params() : inv_imu_selftest.h
- inv_imu_sensor_id_t : inv_imu_driver_advanced.h
- inv_imu_serif_type_t : inv_imu_transport.h
- inv_imu_set_accel_frequency() : inv_imu_driver.h
- inv_imu_set_accel_fsr() : inv_imu_driver.h
- inv_imu_set_accel_ln_bw() : inv_imu_driver.h
- inv_imu_set_accel_lp_avg() : inv_imu_driver.h
- inv_imu_set_accel_mode() : inv_imu_driver.h
- inv_imu_set_config_int() : inv_imu_driver.h
- inv_imu_set_fifo_config() : inv_imu_driver.h
- inv_imu_set_gyro_frequency() : inv_imu_driver.h
- inv_imu_set_gyro_fsr() : inv_imu_driver.h
- inv_imu_set_gyro_ln_bw() : inv_imu_driver.h
- inv_imu_set_gyro_lp_avg() : inv_imu_driver.h
- inv_imu_set_gyro_mode() : inv_imu_driver.h
- inv_imu_set_pin_config_int() : inv_imu_driver.h
- inv_imu_sleep_us() : inv_imu_driver.h
- inv_imu_soft_reset() : inv_imu_driver.h
- INV_IMU_ST_STATUS_FAIL : inv_imu_selftest.h
- INV_IMU_ST_STATUS_NOT_RUN : inv_imu_selftest.h
- INV_IMU_ST_STATUS_SUCCESS : inv_imu_selftest.h
- INV_IMU_WRITE_EDMP_SRAM : inv_imu_edmp.h
- inv_imu_write_reg() : inv_imu_transport.h
- inv_imu_write_reg_t : inv_imu_transport.h
- inv_imu_write_sram() : inv_imu_transport.h
- INV_SENSOR_ACCEL : inv_imu_driver_advanced.h
- INV_SENSOR_EDMP_FF : inv_imu_driver_advanced.h
- INV_SENSOR_EDMP_HIGHG : inv_imu_driver_advanced.h
- INV_SENSOR_EDMP_LOWG : inv_imu_driver_advanced.h
- INV_SENSOR_EDMP_PEDOMETER_COUNT : inv_imu_driver_advanced.h
- INV_SENSOR_EDMP_PEDOMETER_EVENT : inv_imu_driver_advanced.h
- INV_SENSOR_EDMP_R2W_SLEEP : inv_imu_driver_advanced.h
- INV_SENSOR_EDMP_R2W_WAKE : inv_imu_driver_advanced.h
- INV_SENSOR_EDMP_SMD : inv_imu_driver_advanced.h
- INV_SENSOR_EDMP_TAP : inv_imu_driver_advanced.h
- INV_SENSOR_EDMP_TILT : inv_imu_driver_advanced.h
- INV_SENSOR_ES0 : inv_imu_driver_advanced.h
- INV_SENSOR_ES1 : inv_imu_driver_advanced.h
- INV_SENSOR_FSYNC_EVENT : inv_imu_driver_advanced.h
- INV_SENSOR_GYRO : inv_imu_driver_advanced.h
- INV_SENSOR_MAX : inv_imu_driver_advanced.h
- INV_SENSOR_TEMPERATURE : inv_imu_driver_advanced.h
- INVALID_VALUE_FIFO : inv_imu_defs.h
- INVALID_VALUE_FIFO_1B : inv_imu_defs.h
- IOC_PAD_SCENARIO : inv_imu_regmap_le.h
- IOC_PAD_SCENARIO_AUX_OVRD : inv_imu_regmap_le.h
- IOC_PAD_SCENARIO_OVRD : inv_imu_regmap_le.h
- IOC_PAD_SCENARIO_OVRD_INT2_CFG_OVRD_VAL_DRDY_INTR : inv_imu_defs.h
- IOC_PAD_SCENARIO_OVRD_INT2_CFG_OVRD_VAL_INT2 : inv_imu_defs.h
- ioc_pad_scenario_ovrd_pads_int2_cfg_ovrd_val_t : inv_imu_defs.h
- IPREG_BAR_REG_57 : inv_imu_regmap_le.h
- IPREG_BAR_REG_58 : inv_imu_regmap_le.h
- IPREG_BAR_REG_59 : inv_imu_regmap_le.h
- IPREG_BAR_REG_60 : inv_imu_regmap_le.h
- IPREG_BAR_REG_61 : inv_imu_regmap_le.h
- IPREG_BAR_REG_62 : inv_imu_regmap_le.h
- IPREG_MISC : inv_imu_regmap_le.h
- IPREG_SYS1_REG_166 : inv_imu_regmap_le.h
- IPREG_SYS1_REG_166_GYRO_SRC_CTRL_INTERPOLATOR_OFF_FIR_OFF : inv_imu_defs.h
- IPREG_SYS1_REG_166_GYRO_SRC_CTRL_INTERPOLATOR_OFF_FIR_ON : inv_imu_defs.h
- IPREG_SYS1_REG_166_GYRO_SRC_CTRL_INTERPOLATOR_ON_FIR_ON : inv_imu_defs.h
- ipreg_sys1_reg_166_gyro_src_ctrl_sel_t : inv_imu_defs.h
- IPREG_SYS1_REG_168 : inv_imu_regmap_le.h
- IPREG_SYS1_REG_170 : inv_imu_regmap_le.h
- IPREG_SYS1_REG_170_GYRO_LP_AVG_1 : inv_imu_defs.h
- IPREG_SYS1_REG_170_GYRO_LP_AVG_10 : inv_imu_defs.h
- IPREG_SYS1_REG_170_GYRO_LP_AVG_11 : inv_imu_defs.h
- IPREG_SYS1_REG_170_GYRO_LP_AVG_16 : inv_imu_defs.h
- IPREG_SYS1_REG_170_GYRO_LP_AVG_18 : inv_imu_defs.h
- IPREG_SYS1_REG_170_GYRO_LP_AVG_2 : inv_imu_defs.h
- IPREG_SYS1_REG_170_GYRO_LP_AVG_20 : inv_imu_defs.h
- IPREG_SYS1_REG_170_GYRO_LP_AVG_32 : inv_imu_defs.h
- IPREG_SYS1_REG_170_GYRO_LP_AVG_4 : inv_imu_defs.h
- IPREG_SYS1_REG_170_GYRO_LP_AVG_5 : inv_imu_defs.h
- IPREG_SYS1_REG_170_GYRO_LP_AVG_64 : inv_imu_defs.h
- IPREG_SYS1_REG_170_GYRO_LP_AVG_7 : inv_imu_defs.h
- IPREG_SYS1_REG_170_GYRO_LP_AVG_8 : inv_imu_defs.h
- ipreg_sys1_reg_170_gyro_lp_avg_sel_t : inv_imu_defs.h
- IPREG_SYS1_REG_171 : inv_imu_regmap_le.h
- IPREG_SYS1_REG_172 : inv_imu_regmap_le.h
- IPREG_SYS1_REG_172_GYRO_UI_LPFBW_DIV_128 : inv_imu_defs.h
- IPREG_SYS1_REG_172_GYRO_UI_LPFBW_DIV_16 : inv_imu_defs.h
- IPREG_SYS1_REG_172_GYRO_UI_LPFBW_DIV_32 : inv_imu_defs.h
- IPREG_SYS1_REG_172_GYRO_UI_LPFBW_DIV_4 : inv_imu_defs.h
- IPREG_SYS1_REG_172_GYRO_UI_LPFBW_DIV_64 : inv_imu_defs.h
- IPREG_SYS1_REG_172_GYRO_UI_LPFBW_DIV_8 : inv_imu_defs.h
- IPREG_SYS1_REG_172_GYRO_UI_LPFBW_NO_FILTER : inv_imu_defs.h
- ipreg_sys1_reg_172_gyro_ui_lpfbw_sel_t : inv_imu_defs.h
- IPREG_SYS1_REG_173 : inv_imu_regmap_le.h
- IPREG_SYS1_REG_42 : inv_imu_regmap_le.h
- IPREG_SYS1_REG_43 : inv_imu_regmap_le.h
- IPREG_SYS1_REG_56 : inv_imu_regmap_le.h
- IPREG_SYS1_REG_57 : inv_imu_regmap_le.h
- IPREG_SYS1_REG_70 : inv_imu_regmap_le.h
- IPREG_SYS1_REG_71 : inv_imu_regmap_le.h
- IPREG_SYS2_REG_123 : inv_imu_regmap_le.h
- IPREG_SYS2_REG_123_ACCEL_SRC_CTRL_INTERPOLATOR_OFF_FIR_OFF : inv_imu_defs.h
- IPREG_SYS2_REG_123_ACCEL_SRC_CTRL_INTERPOLATOR_OFF_FIR_ON : inv_imu_defs.h
- IPREG_SYS2_REG_123_ACCEL_SRC_CTRL_INTERPOLATOR_ON_FIR_ON : inv_imu_defs.h
- ipreg_sys2_reg_123_accel_src_ctrl_sel_t : inv_imu_defs.h
- IPREG_SYS2_REG_129 : inv_imu_regmap_le.h
- IPREG_SYS2_REG_129_ACCEL_LP_AVG_1 : inv_imu_defs.h
- IPREG_SYS2_REG_129_ACCEL_LP_AVG_10 : inv_imu_defs.h
- IPREG_SYS2_REG_129_ACCEL_LP_AVG_11 : inv_imu_defs.h
- IPREG_SYS2_REG_129_ACCEL_LP_AVG_16 : inv_imu_defs.h
- IPREG_SYS2_REG_129_ACCEL_LP_AVG_18 : inv_imu_defs.h
- IPREG_SYS2_REG_129_ACCEL_LP_AVG_2 : inv_imu_defs.h
- IPREG_SYS2_REG_129_ACCEL_LP_AVG_20 : inv_imu_defs.h
- IPREG_SYS2_REG_129_ACCEL_LP_AVG_32 : inv_imu_defs.h
- IPREG_SYS2_REG_129_ACCEL_LP_AVG_4 : inv_imu_defs.h
- IPREG_SYS2_REG_129_ACCEL_LP_AVG_5 : inv_imu_defs.h
- IPREG_SYS2_REG_129_ACCEL_LP_AVG_64 : inv_imu_defs.h
- IPREG_SYS2_REG_129_ACCEL_LP_AVG_7 : inv_imu_defs.h
- IPREG_SYS2_REG_129_ACCEL_LP_AVG_8 : inv_imu_defs.h
- ipreg_sys2_reg_129_accel_lp_avg_sel_t : inv_imu_defs.h
- IPREG_SYS2_REG_130 : inv_imu_regmap_le.h
- IPREG_SYS2_REG_131 : inv_imu_regmap_le.h
- IPREG_SYS2_REG_131_ACCEL_UI_LPFBW_DIV_128 : inv_imu_defs.h
- IPREG_SYS2_REG_131_ACCEL_UI_LPFBW_DIV_16 : inv_imu_defs.h
- IPREG_SYS2_REG_131_ACCEL_UI_LPFBW_DIV_32 : inv_imu_defs.h
- IPREG_SYS2_REG_131_ACCEL_UI_LPFBW_DIV_4 : inv_imu_defs.h
- IPREG_SYS2_REG_131_ACCEL_UI_LPFBW_DIV_64 : inv_imu_defs.h
- IPREG_SYS2_REG_131_ACCEL_UI_LPFBW_DIV_8 : inv_imu_defs.h
- IPREG_SYS2_REG_131_ACCEL_UI_LPFBW_NO_FILTER : inv_imu_defs.h
- ipreg_sys2_reg_131_accel_ui_lpfbw_t : inv_imu_defs.h
- IPREG_SYS2_REG_132 : inv_imu_regmap_le.h
- IPREG_SYS2_REG_24 : inv_imu_regmap_le.h
- IPREG_SYS2_REG_25 : inv_imu_regmap_le.h
- IPREG_SYS2_REG_32 : inv_imu_regmap_le.h
- IPREG_SYS2_REG_33 : inv_imu_regmap_le.h
- IPREG_SYS2_REG_40 : inv_imu_regmap_le.h
- IPREG_SYS2_REG_41 : inv_imu_regmap_le.h
- IREG_ADDR_15_8 : inv_imu_regmap_le.h
- IREG_ADDR_7_0 : inv_imu_regmap_le.h
- IREG_DATA : inv_imu_regmap_le.h
- ISR_0_7 : inv_imu_regmap_le.h
- ISR_16_23 : inv_imu_regmap_le.h
- ISR_8_15 : inv_imu_regmap_le.h