| ICM45686 eMD driver Documentation of the eMD Driver API

- Main Page
- Related Pages
- Modules
- Classes
- Files

- Class List
- Class Index
- Class Members

Public Attributes | List of all members
i2cm_status_t Struct Reference

`#include <inv_imu_regmap_le.h>`

## Public Attributes
uint8_t | i2cm_busy: 1
uint8_t | i2cm_done: 1
uint8_t | i2cm_timeout_err: 1
uint8_t | i2cm_srst_err: 1
uint8_t | i2cm_scl_err: 1
uint8_t | i2cm_sda_err: 1
uint8_t | resv_1: 2

## Member Data Documentation

## ◆ i2cm_busy

uint8_t i2cm_status_t::i2cm_busy

## ◆ i2cm_done

uint8_t i2cm_status_t::i2cm_done

## ◆ i2cm_scl_err

uint8_t i2cm_status_t::i2cm_scl_err

## ◆ i2cm_sda_err

uint8_t i2cm_status_t::i2cm_sda_err

## ◆ i2cm_srst_err

uint8_t i2cm_status_t::i2cm_srst_err

## ◆ i2cm_timeout_err

uint8_t i2cm_status_t::i2cm_timeout_err

## ◆ resv_1

uint8_t i2cm_status_t::resv_1

The documentation for this struct was generated from the following file:

- inv_imu_regmap_le.h