| ICM45686 eMD driver Documentation of the eMD Driver API

- Main Page
- Related Pages
- Modules
- Classes
- Files

- Class List
- Class Index
- Class Members

Public Attributes | List of all members
status_mask_pin_0_7_t Struct Reference

`#include <inv_imu_regmap_le.h>`

## Public Attributes
uint8_t | int_accel_drdy_pin_0_dis: 1
uint8_t | resv_1: 2
uint8_t | int_ext_odr_drdy_pin_0_dis: 1
uint8_t | resv_2: 1
uint8_t | int_on_demand_pin_0_dis: 1
uint8_t | resv_3: 2

## Member Data Documentation

## ◆ int_accel_drdy_pin_0_dis

uint8_t status_mask_pin_0_7_t::int_accel_drdy_pin_0_dis

## ◆ int_ext_odr_drdy_pin_0_dis

uint8_t status_mask_pin_0_7_t::int_ext_odr_drdy_pin_0_dis

## ◆ int_on_demand_pin_0_dis

uint8_t status_mask_pin_0_7_t::int_on_demand_pin_0_dis

## ◆ resv_1

uint8_t status_mask_pin_0_7_t::resv_1

## ◆ resv_2

uint8_t status_mask_pin_0_7_t::resv_2

## ◆ resv_3

uint8_t status_mask_pin_0_7_t::resv_3

The documentation for this struct was generated from the following file:

- inv_imu_regmap_le.h