| ICM45686 eMD driver Documentation of the eMD Driver API

- Main Page
- Related Pages
- Modules
- Classes
- Files

- Class List
- Class Index
- Class Members

Public Attributes | List of all members
ioc_pad_scenario_t Struct Reference

`#include <inv_imu_regmap_le.h>`

## Public Attributes
uint8_t | aux1_enable: 1
uint8_t | aux1_mode: 2
uint8_t | aux2_enable: 1
uint8_t | pads_int2_cfg: 2
uint8_t | resv_1: 2

## Member Data Documentation

## ◆ aux1_enable

uint8_t ioc_pad_scenario_t::aux1_enable

## ◆ aux1_mode

uint8_t ioc_pad_scenario_t::aux1_mode

## ◆ aux2_enable

uint8_t ioc_pad_scenario_t::aux2_enable

## ◆ pads_int2_cfg

uint8_t ioc_pad_scenario_t::pads_int2_cfg

## ◆ resv_1

uint8_t ioc_pad_scenario_t::resv_1

The documentation for this struct was generated from the following file:

- inv_imu_regmap_le.h