| ICM45686 eMD driver Documentation of the eMD Driver API

- Main Page
- Related Pages
- Modules
- Classes
- Files

- Class List
- Class Index
- Class Members

Public Attributes | List of all members
i2cm_command_0_t Struct Reference

`#include <inv_imu_regmap_le.h>`

## Public Attributes
uint8_t | burstlen_0: 4
uint8_t | r_w_0: 2
uint8_t | ch_sel_0: 1
uint8_t | endflag_0: 1

## Member Data Documentation

## ◆ burstlen_0

uint8_t i2cm_command_0_t::burstlen_0

## ◆ ch_sel_0

uint8_t i2cm_command_0_t::ch_sel_0

## ◆ endflag_0

uint8_t i2cm_command_0_t::endflag_0

## ◆ r_w_0

uint8_t i2cm_command_0_t::r_w_0

The documentation for this struct was generated from the following file:

- inv_imu_regmap_le.h