| ICM45686 eMD driver Documentation of the eMD Driver API

- Main Page
- Related Pages
- Modules
- Classes
- Files

- Class List
- Class Index
- Class Members

- All
- Variables

- a
- b
- c
- d
- e
- f
- g
- h
- i
- l
- n
- o
- p
- r
- s
- t
- u
- v
- w

Here is a list of all class members with links to the classes they belong to:

### - r -

- r2w_en : edmp_apex_en0_t
- r2w_gesture_validity_timeout : inv_imu_edmp_apex_parameters_t
- r2w_gravity_filter_gain : inv_imu_edmp_apex_parameters_t
- r2w_last_gravity_motion_timer : inv_imu_edmp_apex_parameters_t
- r2w_last_gravity_timeout : inv_imu_edmp_apex_parameters_t
- r2w_motion_prev_gravity_timeout : inv_imu_edmp_apex_parameters_t
- r2w_motion_th_angle_cosine : inv_imu_edmp_apex_parameters_t
- r2w_motion_th_timer_fast : inv_imu_edmp_apex_parameters_t
- r2w_motion_th_timer_slow : inv_imu_edmp_apex_parameters_t
- r2w_mounting_matrix : inv_imu_edmp_apex_parameters_t
- r2w_sleep_gesture_delay : inv_imu_edmp_apex_parameters_t
- r2w_sleep_time_out : inv_imu_edmp_apex_parameters_t
- r_w_0 : i2cm_command_0_t
- r_w_1 : i2cm_command_1_t
- r_w_2 : i2cm_command_2_t
- r_w_3 : i2cm_command_3_t
- rd_address_0 : i2cm_dev_profile0_t
- rd_address_1 : i2cm_dev_profile2_t
- read_reg : inv_imu_transport_t
- reserved0 : edmp_apex_en0_t
- reserved1 : edmp_apex_en0_t
- resv_1 : accel_config0_t , dmp_ext_sen_odr_cfg_t , drive_config0_t , drive_config1_t , drive_config2_t , edmp_apex_en1_t , fifo_config2_t , fifo_config3_t , fifo_config4_t , fifo_sram_sleep_t , fs_sel_aux1_t , fs_sel_aux2_t , fsync_config0_t , fsync_config1_t , i2cm_control_t , i2cm_dev_profile1_t , i2cm_dev_profile3_t , i2cm_ext_dev_status_t , i2cm_status_t , int1_config1_t , int1_config2_t , int1_status1_t , int2_config1_t , int2_config2_t , int2_status1_t , int_apex_config1_t , int_apex_status1_t , int_aux2_config_t , int_aux2_status_t , int_i2cm_source_t , int_pulse_min_off_intf0_t , int_pulse_min_off_intf1_t , int_pulse_min_on_intf0_t , int_pulse_min_on_intf1_t , intf_aux_config_t , intf_config0_t , intf_config1_ovrd_t , intf_config_ovrd_aux1_t , intf_config_ovrd_aux2_t , ioc_pad_scenario_aux_ovrd_t , ioc_pad_scenario_ovrd_t , ioc_pad_scenario_t , ipreg_bar_reg_57_t , ipreg_bar_reg_58_t , ipreg_bar_reg_59_t , ipreg_bar_reg_60_t , ipreg_bar_reg_61_t , ipreg_bar_reg_62_t , ipreg_misc_t , ipreg_sys1_reg_166_t , ipreg_sys1_reg_168_t , ipreg_sys1_reg_170_t , ipreg_sys1_reg_171_t , ipreg_sys1_reg_172_t , ipreg_sys1_reg_173_t , ipreg_sys2_reg_123_t , ipreg_sys2_reg_129_t , ipreg_sys2_reg_130_t , ipreg_sys2_reg_131_t , ipreg_sys2_reg_132_t , isr_0_7_t , isr_16_23_t , isr_8_15_t , pwr_mgmt0_t , pwr_mgmt_aux1_t , pwr_mgmt_aux2_t , reg_host_msg_t , reg_misc1_t , reg_misc2_t , rtc_config_t , selftest_t , sifs_i3c_stc_cfg_t , sifs_ixc_error_status_t , smc_control_0_t , smc_control_1_t , sreg_ctrl_t , status_mask_pin_0_7_t , status_mask_pin_16_23_t , status_mask_pin_8_15_t , stc_config_t , tmst_wom_config_t
- resv_2 : edmp_apex_en1_t , fifo_config2_t , i2cm_control_t , int_apex_config1_t , int_apex_status1_t , intf_config0_t , ipreg_bar_reg_57_t , ipreg_bar_reg_58_t , ipreg_bar_reg_59_t , ipreg_bar_reg_60_t , ipreg_bar_reg_61_t , ipreg_bar_reg_62_t , ipreg_misc_t , ipreg_sys1_reg_166_t , isr_0_7_t , isr_16_23_t , isr_8_15_t , reg_host_msg_t , rtc_config_t , sifs_i3c_stc_cfg_t , smc_control_1_t , sreg_ctrl_t , status_mask_pin_0_7_t , status_mask_pin_16_23_t , status_mask_pin_8_15_t , stc_config_t
- resv_3 : i2cm_control_t , ipreg_bar_reg_59_t , isr_0_7_t , isr_16_23_t , isr_8_15_t , status_mask_pin_0_7_t , status_mask_pin_16_23_t , status_mask_pin_8_15_t
- rtc_align : rtc_config_t
- rtc_mode : rtc_config_t