| ICM45686 eMD driver Documentation of the eMD Driver API

- Main Page
- Related Pages
- Modules
- Classes
- Files

- Class List
- Class Index
- Class Members

Public Attributes | List of all members
int_apex_config0_t Struct Reference

`#include <inv_imu_regmap_le.h>`

## Public Attributes
uint8_t | int_status_mask_pin_tap_detect: 1
uint8_t | int_status_mask_pin_high_g_det: 1
uint8_t | int_status_mask_pin_low_g_det: 1
uint8_t | int_status_mask_pin_tilt_det: 1
uint8_t | int_status_mask_pin_step_cnt_ovfl: 1
uint8_t | int_status_mask_pin_step_det: 1
uint8_t | int_status_mask_pin_ff_det: 1
uint8_t | int_status_mask_pin_r2w_wake_det: 1

## Member Data Documentation

## ◆ int_status_mask_pin_ff_det

uint8_t int_apex_config0_t::int_status_mask_pin_ff_det

## ◆ int_status_mask_pin_high_g_det

uint8_t int_apex_config0_t::int_status_mask_pin_high_g_det

## ◆ int_status_mask_pin_low_g_det

uint8_t int_apex_config0_t::int_status_mask_pin_low_g_det

## ◆ int_status_mask_pin_r2w_wake_det

uint8_t int_apex_config0_t::int_status_mask_pin_r2w_wake_det

## ◆ int_status_mask_pin_step_cnt_ovfl

uint8_t int_apex_config0_t::int_status_mask_pin_step_cnt_ovfl

## ◆ int_status_mask_pin_step_det

uint8_t int_apex_config0_t::int_status_mask_pin_step_det

## ◆ int_status_mask_pin_tap_detect

uint8_t int_apex_config0_t::int_status_mask_pin_tap_detect

## ◆ int_status_mask_pin_tilt_det

uint8_t int_apex_config0_t::int_status_mask_pin_tilt_det

The documentation for this struct was generated from the following file:

- inv_imu_regmap_le.h