| ICM42688V eMD Driver 2.0.9 Documentation of the eMD Driver API

- Main Page
- Related Pages
- Modules
- Classes
- Files

- Class List
- Class Index
- Class Members

Public Attributes | List of all members
fifo_header_t Union Reference

Describe the content of the FIFO header. More...

`#include <Icm426xxDefs.h>`

## Public Attributes
unsigned char | Byte
struct {
unsigned char gyro_odr_different: 1
unsigned char accel_odr_different: 1
unsigned char fsync_bit: 1
unsigned char timestamp_bit: 1
unsigned char twentybits_bit: 1
unsigned char gyro_bit: 1
unsigned char accel_bit: 1
unsigned char msg_bit: 1
} | bits

## Detailed Description

Describe the content of the FIFO header.

## Member Data Documentation

## ◆ accel_bit

unsigned char fifo_header_t::accel_bit

## ◆ accel_odr_different

unsigned char fifo_header_t::accel_odr_different

## ◆

struct { ... } fifo_header_t::bits

## ◆ Byte

unsigned char fifo_header_t::Byte

## ◆ fsync_bit

unsigned char fifo_header_t::fsync_bit

## ◆ gyro_bit

unsigned char fifo_header_t::gyro_bit

## ◆ gyro_odr_different

unsigned char fifo_header_t::gyro_odr_different

## ◆ msg_bit

unsigned char fifo_header_t::msg_bit

## ◆ timestamp_bit

unsigned char fifo_header_t::timestamp_bit

## ◆ twentybits_bit

unsigned char fifo_header_t::twentybits_bit

The documentation for this union was generated from the following file:

- Icm426xxDefs.h