| ICM42605 eMD Driver 2.0.9 Documentation of the eMD Driver API

- Main Page
- Related Pages
- Modules
- Classes
- Files

- Class List
- Class Index
- Class Members

Public Attributes | List of all members
inv_icm426xx_tap_parameters_t Struct Reference
APEX driver

Icm426xx TAP inputs parameters definition. More...

`#include <Icm426xxDriver_HL_apex.h>`

## Public Attributes
uint8_t | min_jerk_thr
| Minimum Jerk Threshold. More...
ICM426XX_APEX_CONFIG7_TAP_MAX_PEAK_TOL_t | max_peak_tol
| Maximum peak tolerance. More...
ICM426XX_APEX_CONFIG8_TAP_TMAX_t | tmax
| Tap measurement window. More...
ICM426XX_APEX_CONFIG8_TAP_TAVG_t | tavg
| Energy measumerement window. More...
ICM426XX_APEX_CONFIG8_TAP_TMIN_t | tmin
| Single tap window. More...

## Detailed Description

Icm426xx TAP inputs parameters definition.

## Member Data Documentation

## ◆ max_peak_tol

ICM426XX_APEX_CONFIG7_TAP_MAX_PEAK_TOL_t inv_icm426xx_tap_parameters_t::max_peak_tol

Maximum peak tolerance.

## ◆ min_jerk_thr

uint8_t inv_icm426xx_tap_parameters_t::min_jerk_thr

Minimum Jerk Threshold.

## ◆ tavg

ICM426XX_APEX_CONFIG8_TAP_TAVG_t inv_icm426xx_tap_parameters_t::tavg

Energy measumerement window.

## ◆ tmax

ICM426XX_APEX_CONFIG8_TAP_TMAX_t inv_icm426xx_tap_parameters_t::tmax

Tap measurement window.

## ◆ tmin

ICM426XX_APEX_CONFIG8_TAP_TMIN_t inv_icm426xx_tap_parameters_t::tmin

Single tap window.

The documentation for this struct was generated from the following file:

- Icm426xxDriver_HL_apex.h