| ICM42370P eMD Driver 2.2.7 Documentation of the eMD Driver API

- Main Page
- Related Pages
- Modules
- Classes
- Files

- Class List
- Class Index
- Class Members

- All
- Variables

- a
- b
- c
- d
- e
- f
- h
- i
- l
- m
- n
- p
- r
- s
- t
- w

Here is a list of all class members with links to the classes they belong to:

### - a -

- accel : inv_imu_sensor_event_t
- accel_bit : fifo_header_t
- accel_config0_reg : inv_imu_transport::register_cache
- accel_high_res : inv_imu_sensor_event_t
- accel_odr_different : fifo_header_t
- accel_start_time_us : inv_imu_device
- accel_status : inv_imu_selftest_output_t
- activity_class : APEX_DATA_STEP_ACTIVITY , inv_imu_apex_step_activity
- ax_status : inv_imu_selftest_output_t
- ay_status : inv_imu_selftest_output_t
- az_status : inv_imu_selftest_output_t

### - b -

- bits : fifo_header_t
- Byte : fifo_header_t

### - c -

- context : inv_imu_serif

### - d -

- dmp_is_on : inv_imu_device

### - e -

- endianness_data : inv_imu_device

### - f -

- ff_debounce_duration : inv_imu_apex_parameters_t
- ff_max_duration_cm : inv_imu_apex_parameters_t
- ff_min_duration_cm : inv_imu_apex_parameters_t
- fifo_data : inv_imu_device
- fifo_highres_enabled : inv_imu_device
- fifo_is_used : inv_imu_device

### - h -

- highg_peak_hyst : inv_imu_apex_parameters_t
- highg_peak_th : inv_imu_apex_parameters_t
- highg_samples_th : inv_imu_apex_parameters_t

### - i -

- INV_FF : inv_imu_interrupt_parameter_t
- INV_FIFO_FULL : inv_imu_interrupt_parameter_t
- INV_FIFO_THS : inv_imu_interrupt_parameter_t
- INV_LOWG : inv_imu_interrupt_parameter_t
- INV_SMD : inv_imu_interrupt_parameter_t
- INV_STEP_CNT_OVFL : inv_imu_interrupt_parameter_t
- INV_STEP_DET : inv_imu_interrupt_parameter_t
- INV_TILT_DET : inv_imu_interrupt_parameter_t
- INV_UI_DRDY : inv_imu_interrupt_parameter_t
- INV_UI_FSYNC : inv_imu_interrupt_parameter_t
- INV_WOM_X : inv_imu_interrupt_parameter_t
- INV_WOM_Y : inv_imu_interrupt_parameter_t
- INV_WOM_Z : inv_imu_interrupt_parameter_t

### - l -

- low_energy_amp_th : inv_imu_apex_parameters_t
- lowg_peak_hyst : inv_imu_apex_parameters_t
- lowg_peak_th : inv_imu_apex_parameters_t
- lowg_samples_th : inv_imu_apex_parameters_t

### - m -

- max_read : inv_imu_serif
- max_write : inv_imu_serif
- msg_bit : fifo_header_t

### - n -

- need_mclk_cnt : inv_imu_transport

### - p -

- pedo_amp_th : inv_imu_apex_parameters_t
- pedo_hi_enrgy_th : inv_imu_apex_parameters_t
- pedo_sb_timer_th : inv_imu_apex_parameters_t
- pedo_step_cnt_th : inv_imu_apex_parameters_t
- pedo_step_det_th : inv_imu_apex_parameters_t
- power_save : inv_imu_apex_parameters_t
- power_save_time : inv_imu_apex_parameters_t
- pwr_mgmt0_reg : inv_imu_transport::register_cache

### - r -

- read_reg : inv_imu_serif
- register_cache : inv_imu_transport
- reserved1 : fifo_header_t
- reserved2 : fifo_header_t
- reserved3 : fifo_header_t

### - s -

- sensitivity_mode : inv_imu_apex_parameters_t
- sensor_event_cb : inv_imu_device
- sensor_mask : inv_imu_sensor_event_t
- serif : inv_imu_transport
- serif_type : inv_imu_serif
- smd_sensitivity : inv_imu_apex_parameters_t
- st_control : inv_imu_selftest_parameters_t
- st_num_samples : inv_imu_selftest_parameters_t
- step_cadence : APEX_DATA_STEP_ACTIVITY , inv_imu_apex_step_activity
- step_cnt : APEX_DATA_STEP_ACTIVITY , inv_imu_apex_step_activity

### - t -

- temperature : inv_imu_sensor_event_t
- tilt_wait_time : inv_imu_apex_parameters_t
- timestamp_bit : fifo_header_t
- timestamp_fsync : inv_imu_sensor_event_t
- tmst_config1_reg : inv_imu_transport::register_cache
- transport : inv_imu_device
- twentybits_bit : fifo_header_t

### - w -

- write_reg : inv_imu_serif