| ICM-4268x-V Driver API 1.0.1 ICM-4268x-V Driver API

Public Attributes | List of all members
inv_icm426xx_transport::register_cache Struct Reference

Contains mirrored values of some IP registers. More...

`#include <Icm426xxTransport.h>`

## Public Attributes
uint8_t | intf_cfg_1_reg
| INTF_CONFIG1, Bank: 0, Address: 0x4D.
uint8_t | pwr_mngt_0_reg
| PWR_MGMT_0, Bank: 0, Address: 0x4E.
uint8_t | gyro_cfg_0_reg
| GYRO_CONFIG0, Bank: 0, Address: 0x4F.
uint8_t | accel_cfg_0_reg
| ACCEL_CONFIG0, Bank: 0, Address: 0x50.
uint8_t | tmst_cfg_reg
| TMST_CONFIG, Bank: 0, Address: 0x54.
uint8_t | bank_sel_reg
| MPUREG_REG_BANK_SEL, All banks, Address 0x76.

## Detailed Description

Contains mirrored values of some IP registers.

The documentation for this struct was generated from the following file:

- Icm426xxTransport.h